Data Fields
thscps_test_conn_info_t Struct Reference
BLE Services » Throughput Control Point Client (THSCPS) » Structures

THS connect Information value. More...

`#include <thscps.h>`

## Data Fields
uint16_t | ci
uint16_t | pdu
uint16_t | mtu
uint8_t | tx_phy
uint8_t | rx_phy
int8_t | tx_power
uint8_t | ths_mode

## Detailed Description

THS connect Information value.

## Field Documentation

## ◆ ci

uint16_t thscps_test_conn_info_t::ci

Connect Interval.

## ◆ mtu

uint16_t thscps_test_conn_info_t::mtu

MTU.

## ◆ pdu

uint16_t thscps_test_conn_info_t::pdu

PDU.

## ◆ rx_phy

uint8_t thscps_test_conn_info_t::rx_phy

RX PHY.

## ◆ ths_mode

uint8_t thscps_test_conn_info_t::ths_mode

THS Mode.

## ◆ tx_phy

uint8_t thscps_test_conn_info_t::tx_phy

TX PHY.

## ◆ tx_power

int8_t thscps_test_conn_info_t::tx_power

TX Power.

The documentation for this struct was generated from the following file:

- thscps.h