Macros
I2S Interrupt Definition
Peripheral Driver » HAL Driver » I2S » Defines » I2S Exported Constants

## Macros
#define | I2S_IT_TXFO LL_I2S_INT_TXFO
| TX FIFO write overflow interrupt More...
#define | I2S_IT_TXFE LL_I2S_INT_TXFE
| TX FIFO empty trigger interrupt More...
#define | I2S_IT_RXFO LL_I2S_INT_RXFO
| RX FIFO receive overflow interrupt. More...
#define | I2S_IT_RXDA LL_I2S_INT_RXDA
| RX FIFO data available interrupt More...

## Detailed Description

## Macro Definition Documentation

## ◆ I2S_IT_RXDA

#define I2S_IT_RXDA LL_I2S_INT_RXDA

RX FIFO data available interrupt

Definition at line 262 of file gr55xx_hal_i2s.h.

## ◆ I2S_IT_RXFO

#define I2S_IT_RXFO LL_I2S_INT_RXFO

RX FIFO receive overflow interrupt.

Definition at line 261 of file gr55xx_hal_i2s.h.

## ◆ I2S_IT_TXFE

#define I2S_IT_TXFE LL_I2S_INT_TXFE

TX FIFO empty trigger interrupt

Definition at line 260 of file gr55xx_hal_i2s.h.

## ◆ I2S_IT_TXFO

#define I2S_IT_TXFO LL_I2S_INT_TXFO

TX FIFO write overflow interrupt

Definition at line 259 of file gr55xx_hal_i2s.h.