Macros
Defines
BLE Services » Apple Media Service Client (AMS_C)

## Macros
#define | AMS_C_CONNECTION_MAX
| Maximum number of HRS Client connections. More...
#define | AMS_C_ATTR_COUNT_MAX 256
| The buffer size of command. More...
#define | AMS_C_TRUNCATED_FLAG (0x01<<0)
| Bit of truncated. More...
#define | AMS_SRVC_UUID
| UUID of Apple media service. More...
#define | AMS_CMD_UUID
| UUID of remote command. More...
#define | AMS_ATTR_UPDATE_UUID
| UUID of attribute update. More...
#define | AMS_ATTR_DISPLAY_UUID
| UUID of attribute display. More...

## Detailed Description

## Macro Definition Documentation

## ◆ AMS_ATTR_DISPLAY_UUID

#define AMS_ATTR_DISPLAY_UUID

Value:
0xd7, 0xd5, 0xbb, 0x70, 0xa8, 0xa3, 0xab, 0xa6,\
0xd8, 0x46, 0xab, 0x23, 0x8c, 0xf3, 0xb2, 0xc6

UUID of attribute display.

Definition at line 87 of file ams_c.h.

## ◆ AMS_ATTR_UPDATE_UUID

#define AMS_ATTR_UPDATE_UUID

Value:
0x02, 0xC1, 0x96, 0xBA, 0x92, 0xBB, 0x0C, 0x9A,\
0x1F, 0x41, 0x8D, 0x80, 0xCE, 0xAB, 0x7C, 0x2F

UUID of attribute update.

Definition at line 85 of file ams_c.h.

## ◆ AMS_C_ATTR_COUNT_MAX

#define AMS_C_ATTR_COUNT_MAX 256

The buffer size of command.

Definition at line 78 of file ams_c.h.

## ◆ AMS_C_CONNECTION_MAX

#define AMS_C_CONNECTION_MAX

Value:
(10 < CFG_MAX_CONNECTIONS ?\
10 : CFG_MAX_CONNECTIONS)

Maximum number of HRS Client connections.

Definition at line 77 of file ams_c.h.

## ◆ AMS_C_TRUNCATED_FLAG

#define AMS_C_TRUNCATED_FLAG (0x01<<0)

Bit of truncated.

Definition at line 79 of file ams_c.h.

## ◆ AMS_CMD_UUID

#define AMS_CMD_UUID

Value:
0xc2, 0x51, 0xca, 0xf7, 0x56, 0x0e, 0xdf, 0xb8,\
0x8a, 0x4a, 0xb1, 0x57, 0xd8, 0x81, 0x3c, 0x9b

UUID of remote command.

Definition at line 83 of file ams_c.h.

## ◆ AMS_SRVC_UUID

#define AMS_SRVC_UUID

Value:
0xdc, 0xf8, 0x55, 0xad, 0x02, 0xc5, 0xf4, 0x8e,\
0x3a, 0x43, 0x36, 0x0f, 0x2b, 0x50, 0xd3, 0x89

UUID of Apple media service.

Definition at line 81 of file ams_c.h.