Macros
Defines
BLE Services » FAST_OTA Service (FAST_OTAS)

## Macros
#define | FAST_OTAS_CONNECTION_MAX
| Maximum number of FAST_OTA Service connections. More...
#define | FAST_OTAS_MAX_DATA_LEN 244
| Maximum length of FAST_OTAS characteristic. More...
#define | BLE_UUID_FAST_OTA_SERVICE
| The UUID of FAST_OTA Service for setting advertising data. More...
#define | FAST_OTA_PATTERN_VALUE 0x474f4f44
| The Fast OTA pattern value. More...

## Detailed Description

## Macro Definition Documentation

## ◆ BLE_UUID_FAST_OTA_SERVICE

#define BLE_UUID_FAST_OTA_SERVICE

Value:
0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
0x0A, 0x46, 0x44, 0xD3, 0x01, 0x07, 0xED, 0xA6

The UUID of FAST_OTA Service for setting advertising data.

Definition at line 77 of file fast_otas.h.

## ◆ FAST_OTA_PATTERN_VALUE

#define FAST_OTA_PATTERN_VALUE 0x474f4f44

The Fast OTA pattern value.

Definition at line 79 of file fast_otas.h.

## ◆ FAST_OTAS_CONNECTION_MAX

#define FAST_OTAS_CONNECTION_MAX

Value:
(10 < CFG_MAX_CONNECTIONS ?\
10 : CFG_MAX_CONNECTIONS)

Maximum number of FAST_OTA Service connections.

Definition at line 74 of file fast_otas.h.

## ◆ FAST_OTAS_MAX_DATA_LEN

#define FAST_OTAS_MAX_DATA_LEN 244

Maximum length of FAST_OTAS characteristic.

Definition at line 75 of file fast_otas.h.