Modules | Macros
Defines
BLE Services » Body Composition Service (BCS)

## Modules
| Measurement packets index
| BCS Measurement Packet Index.
| Characteristics Mask
| Bit masks for the initialization of bcs_init_t::char_mask.

## Macros
#define | BCS_CONNECTION_MAX
| Maximum number of Body Composition Service connections. More...
#define | BCS_MEAS_VAL_LEN_MAX 20
| Maximum length of BC Measurment value. More...
#define | BCS_FEAT_VAL_LEN_MAX 4
| Maximum length of BC Feature value. More...
#define | INDI_PAYLOAD_HEADER_LEN 3
| The length of indication payload header. More...
#define | BCS_CACHE_MEAS_NUM_MAX 25
| Maximum number of cache muasurements value for each user. More...
#define | BCS_MEAS_UNSUCCESS 0xFFFF
| Measurement unsuccessful. More...

## Detailed Description

## Macro Definition Documentation

## ◆ BCS_CACHE_MEAS_NUM_MAX

#define BCS_CACHE_MEAS_NUM_MAX 25

Maximum number of cache muasurements value for each user.

Definition at line 95 of file bcs.h.

## ◆ BCS_CONNECTION_MAX

#define BCS_CONNECTION_MAX

Value:
(10 < CFG_MAX_CONNECTIONS ?\
10 : CFG_MAX_CONNECTIONS)

Maximum number of Body Composition Service connections.

Definition at line 74 of file bcs.h.

## ◆ BCS_FEAT_VAL_LEN_MAX

#define BCS_FEAT_VAL_LEN_MAX 4

Maximum length of BC Feature value.

Definition at line 76 of file bcs.h.

## ◆ BCS_MEAS_UNSUCCESS

#define BCS_MEAS_UNSUCCESS 0xFFFF

Measurement unsuccessful.

Definition at line 97 of file bcs.h.

## ◆ BCS_MEAS_VAL_LEN_MAX

#define BCS_MEAS_VAL_LEN_MAX 20

Maximum length of BC Measurment value.

Definition at line 75 of file bcs.h.

## ◆ INDI_PAYLOAD_HEADER_LEN

#define INDI_PAYLOAD_HEADER_LEN 3

The length of indication payload header.

Definition at line 78 of file bcs.h.