Macros
MicroWire Control
Peripheral Driver » LL Driver » SPI » Defines » SPI Exported Constants

## Macros
#define | LL_SSI_MICROWIRE_HANDSHAKE_DIS 0x00000000UL
| Enable Handshake for Microwire transfer More...
#define | LL_SSI_MICROWIRE_HANDSHAKE_EN (1UL << SSI_MWC_MHS_Pos)
| Disable Handshake for Microwire transfer. More...
#define | LL_SSI_MICROWIRE_RX 0x00000000UL
| Rx mode. More...
#define | LL_SSI_MICROWIRE_TX (1UL << SSI_MWC_MDD_Pos)
| Tx mode. More...
#define | LL_SSI_MICROWIRE_NON_SEQUENTIAL 0x00000000UL
| Non-sequential for Microwire transfer More...
#define | LL_SSI_MICROWIRE_SEQUENTIAL (1UL << SSI_MWC_MWMOD_Pos)
| Sequential for Microwire transfer More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_SSI_MICROWIRE_HANDSHAKE_DIS

#define LL_SSI_MICROWIRE_HANDSHAKE_DIS 0x00000000UL

Enable Handshake for Microwire transfer

Definition at line 351 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_MICROWIRE_HANDSHAKE_EN

#define LL_SSI_MICROWIRE_HANDSHAKE_EN (1UL << SSI_MWC_MHS_Pos)

Disable Handshake for Microwire transfer.

Definition at line 352 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_MICROWIRE_NON_SEQUENTIAL

#define LL_SSI_MICROWIRE_NON_SEQUENTIAL 0x00000000UL

Non-sequential for Microwire transfer

Definition at line 357 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_MICROWIRE_RX

#define LL_SSI_MICROWIRE_RX 0x00000000UL

Rx mode.

Rx transfer at Microwire mode

Definition at line 354 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_MICROWIRE_SEQUENTIAL

#define LL_SSI_MICROWIRE_SEQUENTIAL (1UL << SSI_MWC_MWMOD_Pos)

Sequential for Microwire transfer

Definition at line 358 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_MICROWIRE_TX

#define LL_SSI_MICROWIRE_TX (1UL << SSI_MWC_MDD_Pos)

Tx mode.

Tx transfer at Microwire mode

Definition at line 355 of file gr55xx_ll_spi.h.