Enumerations
HAL PWM state
Peripheral Driver » HAL Driver » PWM » Enumerations

## Enumerations
enum | hal_pwm_state_t { HAL_PWM_STATE_RESET = 0x00, HAL_PWM_STATE_READY = 0x01, HAL_PWM_STATE_BUSY = 0x02, HAL_PWM_STATE_ERROR = 0x04 }
| HAL PWM State Enumerations definition. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ hal_pwm_state_t

enum hal_pwm_state_t

HAL PWM State Enumerations definition.

Enumerator
HAL_PWM_STATE_RESET | Peripheral is not initialized or disabled
HAL_PWM_STATE_READY | Peripheral is initialized and ready for use.
HAL_PWM_STATE_BUSY | An internal process is ongoing
HAL_PWM_STATE_ERROR | Reception process is ongoing

Definition at line 75 of file gr55xx_hal_pwm.h.