Macros
Attribute Permission Value Position
BLE » Generic Attribute Profile (GATT) » Generic Attribute Profile (GATT) Server » Defines

## Macros
#define | READ_POS (0x00)
| Bit position of read permission. More...
#define | WRITE_POS (0x02)
| Bit position of write permission. More...
#define | INDICATE_POS (0x04)
| Bit position of indicate bit. More...
#define | NOTIFY_POS (0x06)
| Bit position of notify bit. More...

## Detailed Description

## Macro Definition Documentation

## ◆ INDICATE_POS

#define INDICATE_POS (0x04)

Bit position of indicate bit.

Used by INDICATE_PERM.

Definition at line 89 of file ble_gatts.h.

## ◆ NOTIFY_POS

#define NOTIFY_POS (0x06)

Bit position of notify bit.

Used by NOTIFY_PERM.

Definition at line 90 of file ble_gatts.h.

## ◆ READ_POS

#define READ_POS (0x00)

Bit position of read permission.

Used by READ_PERM.

Definition at line 87 of file ble_gatts.h.

## ◆ WRITE_POS

#define WRITE_POS (0x02)

Bit position of write permission.

Used by WRITE_CMD_PERM, WRITE_REQ_PERM, WRITE_SIGNED_PERM.

Definition at line 88 of file ble_gatts.h.