Macros
Address bytes in command
Peripheral Driver » LL Driver » XQSPI » Defines » XQSPI Exported Constants

## Macros
#define | LL_XQSPI_XIP_ADDR_3BYTES 0x00000000UL
| Address command is 3 bytes More...
#define | LL_XQSPI_XIP_ADDR_4BYTES XQSPI_XIP_CFG_ADDR4
| Address command is 4 bytes More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_XQSPI_XIP_ADDR_3BYTES

#define LL_XQSPI_XIP_ADDR_3BYTES 0x00000000UL

Address command is 3 bytes

Definition at line 162 of file gr55xx_ll_xqspi.h.

## ◆ LL_XQSPI_XIP_ADDR_4BYTES

#define LL_XQSPI_XIP_ADDR_4BYTES XQSPI_XIP_CFG_ADDR4

Address command is 4 bytes

Definition at line 163 of file gr55xx_ll_xqspi.h.