Macros
Power States Defines
Peripheral Driver » LL Driver » ISO7816 » Defines » ISO7816 Exported Constants

## Macros
#define | LL_ISO7816_PWR_STATE_OFF (0x0UL << ISO7816_STAT_PWR_STAT_POS)
| Off More...
#define | LL_ISO7816_PWR_STATE_PWRUP_VCC (0x1UL << ISO7816_STAT_PWR_STAT_POS)
| Power up VCC More...
#define | LL_ISO7816_PWR_STATE_PWRUP_RST (0x2UL << ISO7816_STAT_PWR_STAT_POS)
| Power up reset More...
#define | LL_ISO7816_PWR_STATE_PWRDN_RST (0x3UL << ISO7816_STAT_PWR_STAT_POS)
| Power Down reset More...
#define | LL_ISO7816_PWR_STATE_PWRDN_VCC (0x4UL << ISO7816_STAT_PWR_STAT_POS)
| Power Down VCC More...
#define | LL_ISO7816_PWR_STATE_STOP_PRE (0x5UL << ISO7816_STAT_PWR_STAT_POS)
| Preparing Clock Stop More...
#define | LL_ISO7816_PWR_STATE_STOP (0x6UL << ISO7816_STAT_PWR_STAT_POS)
| Clock Stopped More...
#define | LL_ISO7816_PWR_STATE_STOP_POST (0x7UL << ISO7816_STAT_PWR_STAT_POS)
| Exiting Clock Stop More...
#define | LL_ISO7816_PWR_STATE_IDLE (0x8UL << ISO7816_STAT_PWR_STAT_POS)
| Idle More...
#define | LL_ISO7816_PWR_STATE_RX_TS0 (0x9UL << ISO7816_STAT_PWR_STAT_POS)
| RX TS Character More...
#define | LL_ISO7816_PWR_STATE_RX_TS1 (0xAUL << ISO7816_STAT_PWR_STAT_POS)
| RX TS Character More...
#define | LL_ISO7816_PWR_STATE_RX (0xBUL << ISO7816_STAT_PWR_STAT_POS)
| Receive More...
#define | LL_ISO7816_PWR_STATE_TX (0xCUL << ISO7816_STAT_PWR_STAT_POS)
| Transmit More...
#define | LL_ISO7816_PWR_STATE_TX_RX (0xDUL << ISO7816_STAT_PWR_STAT_POS)
| Transmit and Receive More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_ISO7816_PWR_STATE_IDLE

#define LL_ISO7816_PWR_STATE_IDLE (0x8UL << ISO7816_STAT_PWR_STAT_POS)

Idle

Definition at line 151 of file gr55xx_ll_iso7816.h.

## ◆ LL_ISO7816_PWR_STATE_OFF

#define LL_ISO7816_PWR_STATE_OFF (0x0UL << ISO7816_STAT_PWR_STAT_POS)

Off

Definition at line 143 of file gr55xx_ll_iso7816.h.

## ◆ LL_ISO7816_PWR_STATE_PWRDN_RST

#define LL_ISO7816_PWR_STATE_PWRDN_RST (0x3UL << ISO7816_STAT_PWR_STAT_POS)

Power Down reset

Definition at line 146 of file gr55xx_ll_iso7816.h.

## ◆ LL_ISO7816_PWR_STATE_PWRDN_VCC

#define LL_ISO7816_PWR_STATE_PWRDN_VCC (0x4UL << ISO7816_STAT_PWR_STAT_POS)

Power Down VCC

Definition at line 147 of file gr55xx_ll_iso7816.h.

## ◆ LL_ISO7816_PWR_STATE_PWRUP_RST

#define LL_ISO7816_PWR_STATE_PWRUP_RST (0x2UL << ISO7816_STAT_PWR_STAT_POS)

Power up reset

Definition at line 145 of file gr55xx_ll_iso7816.h.

## ◆ LL_ISO7816_PWR_STATE_PWRUP_VCC

#define LL_ISO7816_PWR_STATE_PWRUP_VCC (0x1UL << ISO7816_STAT_PWR_STAT_POS)

Power up VCC

Definition at line 144 of file gr55xx_ll_iso7816.h.

## ◆ LL_ISO7816_PWR_STATE_RX

#define LL_ISO7816_PWR_STATE_RX (0xBUL << ISO7816_STAT_PWR_STAT_POS)

Receive

Definition at line 154 of file gr55xx_ll_iso7816.h.

## ◆ LL_ISO7816_PWR_STATE_RX_TS0

#define LL_ISO7816_PWR_STATE_RX_TS0 (0x9UL << ISO7816_STAT_PWR_STAT_POS)

RX TS Character

Definition at line 152 of file gr55xx_ll_iso7816.h.

## ◆ LL_ISO7816_PWR_STATE_RX_TS1

#define LL_ISO7816_PWR_STATE_RX_TS1 (0xAUL << ISO7816_STAT_PWR_STAT_POS)

RX TS Character

Definition at line 153 of file gr55xx_ll_iso7816.h.

## ◆ LL_ISO7816_PWR_STATE_STOP

#define LL_ISO7816_PWR_STATE_STOP (0x6UL << ISO7816_STAT_PWR_STAT_POS)

Clock Stopped

Definition at line 149 of file gr55xx_ll_iso7816.h.

## ◆ LL_ISO7816_PWR_STATE_STOP_POST

#define LL_ISO7816_PWR_STATE_STOP_POST (0x7UL << ISO7816_STAT_PWR_STAT_POS)

Exiting Clock Stop

Definition at line 150 of file gr55xx_ll_iso7816.h.

## ◆ LL_ISO7816_PWR_STATE_STOP_PRE

#define LL_ISO7816_PWR_STATE_STOP_PRE (0x5UL << ISO7816_STAT_PWR_STAT_POS)

Preparing Clock Stop

Definition at line 148 of file gr55xx_ll_iso7816.h.

## ◆ LL_ISO7816_PWR_STATE_TX

#define LL_ISO7816_PWR_STATE_TX (0xCUL << ISO7816_STAT_PWR_STAT_POS)

Transmit

Definition at line 155 of file gr55xx_ll_iso7816.h.

## ◆ LL_ISO7816_PWR_STATE_TX_RX

#define LL_ISO7816_PWR_STATE_TX_RX (0xDUL << ISO7816_STAT_PWR_STAT_POS)

Transmit and Receive

Definition at line 156 of file gr55xx_ll_iso7816.h.