Macros
Defines
BLE Services » OTA Service (OTAS)

## Macros
#define | OTAS_CONNECTION_MAX
| Maximum number of OTA Service connections. More...
#define | OTAS_MAX_DATA_LEN 244
| Maximum length of OTAS characteristic. More...
#define | BLE_UUID_OTA_SERVICE
| The UUID of OTA Service for setting advertising data. More...
#define | OTAS_CTRL_ENTER_DFU 0x474f4f44
| OTAS enter DFU control. More...

## Detailed Description

## Macro Definition Documentation

## ◆ BLE_UUID_OTA_SERVICE

#define BLE_UUID_OTA_SERVICE

Value:
0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
0x0A, 0x46, 0x44, 0xD3, 0x01, 0x04, 0xED, 0xA6

The UUID of OTA Service for setting advertising data.

Definition at line 77 of file otas.h.

## ◆ OTAS_CONNECTION_MAX

#define OTAS_CONNECTION_MAX

Value:
(10 < CFG_MAX_CONNECTIONS ?\
10 : CFG_MAX_CONNECTIONS)

Maximum number of OTA Service connections.

Definition at line 74 of file otas.h.

## ◆ OTAS_CTRL_ENTER_DFU

#define OTAS_CTRL_ENTER_DFU 0x474f4f44

OTAS enter DFU control.

Definition at line 78 of file otas.h.

## ◆ OTAS_MAX_DATA_LEN

#define OTAS_MAX_DATA_LEN 244

Maximum length of OTAS characteristic.

Definition at line 75 of file otas.h.