Macros
I2S Clock Source
Peripheral Driver » HAL Driver » I2S » Defines » I2S Exported Constants

## Macros
#define | I2S_CLOCK_SRC_96M LL_I2S_CLOCK_SRC_96M
| Inactive state of SCLK is low More...
#define | I2S_CLOCK_SRC_32M LL_I2S_CLOCK_SRC_32M
| Inactive state of SCLK is high. More...

## Detailed Description

## Macro Definition Documentation

## ◆ I2S_CLOCK_SRC_32M

#define I2S_CLOCK_SRC_32M LL_I2S_CLOCK_SRC_32M

Inactive state of SCLK is high.

Definition at line 237 of file gr55xx_hal_i2s.h.

## ◆ I2S_CLOCK_SRC_96M

#define I2S_CLOCK_SRC_96M LL_I2S_CLOCK_SRC_96M

Inactive state of SCLK is low

Definition at line 236 of file gr55xx_hal_i2s.h.