Macros
Action state
Peripheral Driver » HAL Driver » ISO7816 » Defines » ISO7816 Exported Constants

## Macros
#define | HAL_ISO7816_ACTION_NONE LL_ISO7816_ACTION_NONE
| Do Nothing. More...
#define | HAL_ISO7816_ACTION_OFF LL_ISO7816_ACTION_OFF
| Switch Off. More...
#define | HAL_ISO7816_ACTION_STOPCLK LL_ISO7816_ACTION_STOPCLK
| Stop the clock. More...
#define | HAL_ISO7816_ACTION_ON LL_ISO7816_ACTION_ON
| Switch on and receive ATR. More...
#define | HAL_ISO7816_ACTION_WARMRST LL_ISO7816_ACTION_WARMRST
| Trigger warm reset and receive ATR. More...
#define | HAL_ISO7816_ACTION_RX LL_ISO7816_ACTION_RX
| Receive. More...
#define | HAL_ISO7816_ACTION_TX LL_ISO7816_ACTION_TX
| Transmit. More...
#define | HAL_ISO7816_ACTION_TXRX LL_ISO7816_ACTION_TXRX
| Transmit, followed by RX. More...

## Detailed Description

## Macro Definition Documentation

## ◆ HAL_ISO7816_ACTION_NONE

#define HAL_ISO7816_ACTION_NONE LL_ISO7816_ACTION_NONE

Do Nothing.

Definition at line 200 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_ACTION_OFF

#define HAL_ISO7816_ACTION_OFF LL_ISO7816_ACTION_OFF

Switch Off.

Definition at line 201 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_ACTION_ON

#define HAL_ISO7816_ACTION_ON LL_ISO7816_ACTION_ON

Switch on and receive ATR.

Definition at line 203 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_ACTION_RX

#define HAL_ISO7816_ACTION_RX LL_ISO7816_ACTION_RX

Receive.

Definition at line 205 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_ACTION_STOPCLK

#define HAL_ISO7816_ACTION_STOPCLK LL_ISO7816_ACTION_STOPCLK

Stop the clock.

Definition at line 202 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_ACTION_TX

#define HAL_ISO7816_ACTION_TX LL_ISO7816_ACTION_TX

Transmit.

Definition at line 206 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_ACTION_TXRX

#define HAL_ISO7816_ACTION_TXRX LL_ISO7816_ACTION_TXRX

Transmit, followed by RX.

Definition at line 207 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_ACTION_WARMRST

#define HAL_ISO7816_ACTION_WARMRST LL_ISO7816_ACTION_WARMRST

Trigger warm reset and receive ATR.

Definition at line 204 of file gr55xx_hal_iso7816.h.