Macros
Defines
BLE Services » Reference Time Update Service (RTUS)

## Macros
#define | RTUS_CONNECTION_MAX
| Maximum number of RTUS connections. More...
#define | RTUS_CTRL_PT_VAL_LEN 1
| Length of Time Update Control Point value. More...
#define | RTUS_UPDATE_STATE_VAL_LEN 2
| Length of Time Update State value. More...
#define | RTUS_CHAR_FULL 0x1f
| Bit mask for mandatory characteristic in RTUS. More...

## Detailed Description

## Macro Definition Documentation

## ◆ RTUS_CHAR_FULL

#define RTUS_CHAR_FULL 0x1f

Bit mask for mandatory characteristic in RTUS.

Definition at line 73 of file rtus.h.

## ◆ RTUS_CONNECTION_MAX

#define RTUS_CONNECTION_MAX

Value:
(10 < CFG_MAX_CONNECTIONS ?\
10 : CFG_MAX_CONNECTIONS)

Maximum number of RTUS connections.

Definition at line 70 of file rtus.h.

## ◆ RTUS_CTRL_PT_VAL_LEN

#define RTUS_CTRL_PT_VAL_LEN 1

Length of Time Update Control Point value.

Definition at line 71 of file rtus.h.

## ◆ RTUS_UPDATE_STATE_VAL_LEN

#define RTUS_UPDATE_STATE_VAL_LEN 2

Length of Time Update State value.

Definition at line 72 of file rtus.h.