Macros
I2S Clock Source
Peripheral Driver » LL Driver » I2S » Defines » I2S Exported Constants

## Macros
#define | LL_I2S_CLOCK_SRC_96M (0x00000000UL)
| I2S clock source select: 96M More...
#define | LL_I2S_CLOCK_SRC_32M (1UL << 18)
| I2S clock source select: 32M More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_I2S_CLOCK_SRC_32M

#define LL_I2S_CLOCK_SRC_32M (1UL << 18)

I2S clock source select: 32M

Definition at line 147 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_CLOCK_SRC_96M

#define LL_I2S_CLOCK_SRC_96M (0x00000000UL)

I2S clock source select: 96M

Definition at line 146 of file gr55xx_ll_i2s.h.