Enumerations
Enumerations
BLE Services » Battery Service Client (BAS_C)

## Enumerations
enum | bas_c_evt_type_t { BAS_C_EVT_INVALID, BAS_C_EVT_DISCOVERY_COMPLETE, BAS_C_EVT_DISCOVERY_FAIL, BAS_C_EVT_BAT_LEVEL_NTF_SET_SUCCESS, BAS_C_EVT_BAT_LEVEL_NTF_SET_ERR, BAS_C_EVT_BAT_LEVE_RECEIVE }
| Battery Service Client event type. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ bas_c_evt_type_t

enum bas_c_evt_type_t

Battery Service Client event type.

Enumerator
BAS_C_EVT_INVALID | BAS Client invalid event.
BAS_C_EVT_DISCOVERY_COMPLETE | BAS Client has found BAS service and its characteristics.
BAS_C_EVT_DISCOVERY_FAIL | BAS Client found BAS service failed because of invalid operation or no found at the peer.
BAS_C_EVT_BAT_LEVEL_NTF_SET_SUCCESS | BAS Client has enabled Notification of Battery Level characteristics.
BAS_C_EVT_BAT_LEVEL_NTF_SET_ERR | Error occured when BAS Client set Notification of Battery Level characteristics.
BAS_C_EVT_BAT_LEVE_RECEIVE | BAS Client has received Battery Level value (Read or Notification from peer).

Definition at line 79 of file bas_c.h.