Macros
Resistor Enable
Peripheral Driver » LL Driver » GPIO » Defines » GPIO Private Macros

## Macros
#define | LL_GPIO_RE_N_Pos 0
| Resistor Enable bits position. More...
#define | LL_GPIO_RE_N_Msk (0x1U << LL_GPIO_RE_N_Pos)
| Resistor Enable bits mask More...
#define | LL_GPIO_RE_N LL_GPIO_RE_N_Msk
| Resistor Enable bits More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_GPIO_RE_N

#define LL_GPIO_RE_N LL_GPIO_RE_N_Msk

Resistor Enable bits

Definition at line 266 of file gr55xx_ll_gpio.h.

## ◆ LL_GPIO_RE_N_Msk

#define LL_GPIO_RE_N_Msk (0x1U << LL_GPIO_RE_N_Pos)

Resistor Enable bits mask

Definition at line 265 of file gr55xx_ll_gpio.h.

## ◆ LL_GPIO_RE_N_Pos

#define LL_GPIO_RE_N_Pos 0

Resistor Enable bits position.

Definition at line 264 of file gr55xx_ll_gpio.h.