### - a -

- ADC_CLK_16M : gr55xx_hal_adc.h
- ADC_CLK_1M : gr55xx_hal_adc.h
- ADC_CLK_1P6M : gr55xx_hal_adc.h
- ADC_CLK_2M : gr55xx_hal_adc.h
- ADC_CLK_4M : gr55xx_hal_adc.h
- ADC_CLK_8M : gr55xx_hal_adc.h
- ADC_DEFAULT_CONFIG : gr55xx_hal_adc.h
- ADC_INPUT_DIFFERENTIAL : gr55xx_hal_adc.h
- ADC_INPUT_SINGLE : gr55xx_hal_adc.h
- ADC_INPUT_SRC_BAT : gr55xx_hal_adc.h
- ADC_INPUT_SRC_IO0 : gr55xx_hal_adc.h
- ADC_INPUT_SRC_IO1 : gr55xx_hal_adc.h
- ADC_INPUT_SRC_IO2 : gr55xx_hal_adc.h
- ADC_INPUT_SRC_IO3 : gr55xx_hal_adc.h
- ADC_INPUT_SRC_IO4 : gr55xx_hal_adc.h
- ADC_INPUT_SRC_REF : gr55xx_hal_adc.h
- ADC_INPUT_SRC_TMP : gr55xx_hal_adc.h
- ADC_REF_SRC_BUF_INT : gr55xx_hal_adc.h
- ADC_REF_SRC_IO0 : gr55xx_hal_adc.h
- ADC_REF_SRC_IO1 : gr55xx_hal_adc.h
- ADC_REF_SRC_IO2 : gr55xx_hal_adc.h
- ADC_REF_SRC_IO3 : gr55xx_hal_adc.h
- ADC_REF_VALUE_0P8 : gr55xx_hal_adc.h
- ADC_REF_VALUE_1P2 : gr55xx_hal_adc.h
- ADC_REF_VALUE_1P6 : gr55xx_hal_adc.h
- AES_BLOCK_MAX : gr55xx_hal_aes.h
- AES_BLOCKSIZE_BITS : gr55xx_hal_aes.h
- AES_BLOCKSIZE_BYTES : gr55xx_hal_aes.h
- AES_BLOCKSIZE_WORDS : gr55xx_hal_aes.h
- AES_CHAININGMODE_CBC : gr55xx_hal_aes.h
- AES_CHAININGMODE_ECB : gr55xx_hal_aes.h
- AES_FLAG_DATAREADY : gr55xx_hal_aes.h
- AES_FLAG_DMA_DONE : gr55xx_hal_aes.h
- AES_FLAG_DMA_ERR : gr55xx_hal_aes.h
- AES_FLAG_KEY_VALID : gr55xx_hal_aes.h
- AES_IT_DONE : gr55xx_hal_aes.h
- AES_KEYSIZE_128BITS : gr55xx_hal_aes.h
- AES_KEYSIZE_192BITS : gr55xx_hal_aes.h
- AES_KEYSIZE_256BITS : gr55xx_hal_aes.h
- AES_OPERATION_MODE_DECRYPT : gr55xx_hal_aes.h
- AES_OPERATION_MODE_ENCRYPT : gr55xx_hal_aes.h
- AGS_CHAR_FULL : ags.h
- AGS_CHAR_MANDATORY : ags.h
- AGS_CONNECTION_MAX : ags.h
- AGS_HEADER_ACK_PAYLOAD_LEN : ags.h
- AGS_HEADER_ACK_RES_1 : ags.h
- AGS_HEADER_ACK_RES_2 : ags.h
- AGS_HEADER_FIRST_RES : ags.h
- AGS_PAIR_ADV_FLAG : ags.h
- AGS_RECONNECT_ADV_FLAG : ags.h
- AGS_RX_VAL_LEN_MAX : ags.h
- AGS_SERVICE_UUID : ags.h
- AGS_TX_VAL_LEN_MAX : ags.h
- AMS_ATTR_DISPLAY_UUID : ams_c.h
- AMS_ATTR_UPDATE_UUID : ams_c.h
- AMS_C_ATTR_COUNT_MAX : ams_c.h
- AMS_C_CONNECTION_MAX : ams_c.h
- AMS_C_TRUNCATED_FLAG : ams_c.h
- AMS_CMD_UUID : ams_c.h
- AMS_SRVC_UUID : ams_c.h
- ANCS_ATTR : ancs_protocol.h
- ANCS_ATTR_MAXLEN : ancs_protocol.h
- ANCS_C_CONNECTION_MAX : ancs_c.h
- ANCS_CONTROL_POINT_UUID : ancs_c.h
- ANCS_DATA_SOURCE_UUID : ancs_c.h
- ANCS_NTF_SOURCE_UUID : ancs_c.h
- ANCS_SRVC_UUID : ancs_c.h
- ANS_ALERT_NTF_CTRL_PT_VAL_LEN : ans.h
- ANS_ALL_CAT_SUP : ans.h , ans_c.h
- ANS_C_ALERT_NTF_CTRL_PT_VAL_LEN : ans_c.h
- ANS_C_CONNECTION_MAX : ans_c.h
- ANS_C_ERROR_CMD_NOT_SUP : ans_c.h
- ANS_C_UTF_8_STR_LEN_MAX : ans_c.h
- ANS_CALL_SUP : ans.h , ans_c.h
- ANS_CONNECTION_MAX : ans.h
- ANS_EMAIL_SUP : ans.h , ans_c.h
- ANS_ERROR_CMD_NOT_SUP : ans.h
- ANS_HG_PRIO_ALERT_SUP : ans.h , ans_c.h
- ANS_INSTANT_MES : ans.h , ans_c.h
- ANS_MISSED_CALL_SUP : ans.h , ans_c.h
- ANS_NEWS_ALERT_VAL_LEN : ans.h
- ANS_NEWS_SUP : ans.h , ans_c.h
- ANS_SCHEDULE_SUP : ans.h , ans_c.h
- ANS_SMPL_ALERT_SUP : ans.h , ans_c.h
- ANS_SMS_MMS_SUP : ans.h , ans_c.h
- ANS_SUP_NEW_ALERT_CAT_VAL_LEN : ans.h
- ANS_SUP_UNREAD_ALERT_CAT_VAL_LEN : ans.h
- ANS_UNREAD_ALERT_STA_VAL_LEN : ans.h
- ANS_UTF_8_STR_LEN_MAX : ans.h
- ANS_VOICE_MAIL_SUP : ans.h , ans_c.h
- AON_GPIO_DEFAULT_CONFIG : gr55xx_hal_aon_gpio.h
- AON_GPIO_MODE_INPUT : gr55xx_hal_aon_gpio.h
- AON_GPIO_MODE_IT_FALLING : gr55xx_hal_aon_gpio.h
- AON_GPIO_MODE_IT_HIGH : gr55xx_hal_aon_gpio.h
- AON_GPIO_MODE_IT_LOW : gr55xx_hal_aon_gpio.h
- AON_GPIO_MODE_IT_RISING : gr55xx_hal_aon_gpio.h
- AON_GPIO_MODE_MUX : gr55xx_hal_aon_gpio.h
- AON_GPIO_MODE_OUTPUT : gr55xx_hal_aon_gpio.h
- AON_GPIO_MUX_0 : gr55xx_hal_aon_gpio_ex.h
- AON_GPIO_MUX_1 : gr55xx_hal_aon_gpio_ex.h
- AON_GPIO_MUX_2 : gr55xx_hal_aon_gpio_ex.h
- AON_GPIO_MUX_3 : gr55xx_hal_aon_gpio_ex.h
- AON_GPIO_MUX_4 : gr55xx_hal_aon_gpio_ex.h
- AON_GPIO_MUX_5 : gr55xx_hal_aon_gpio_ex.h
- AON_GPIO_MUX_6 : gr55xx_hal_aon_gpio_ex.h
- AON_GPIO_MUX_7 : gr55xx_hal_aon_gpio_ex.h
- AON_GPIO_NOPULL : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_0 : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_1 : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_2 : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_3 : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_4 : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_5 : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_6 : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_7 : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_ALL : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_MASK : gr55xx_hal_aon_gpio.h
- AON_GPIO_PULLDOWN : gr55xx_hal_aon_gpio.h
- AON_GPIO_PULLUP : gr55xx_hal_aon_gpio.h
- APP_AON_IO_PIN_ALL : app_io.h
- APP_AON_IO_PIN_MASK : app_io.h
- APP_DRIVER_ADC_WAPEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_AES_WAPEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_COMP_WAPEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_DMA_WAPEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_DUAL_TIM_WAPEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_GPIOTE_WAPEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_HMAC_WAPEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_I2C_WAPEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_I2S_WAPEUP_PRIORITY : app_drv_config.h
- app_driver_mutex_deinit : app_rtos_cfg.h
- app_driver_mutex_init : app_rtos_cfg.h
- app_driver_mutex_pend : app_rtos_cfg.h
- app_driver_mutex_post : app_rtos_cfg.h
- APP_DRIVER_PWM_WAPEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_QSPI_WAPEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_RNG_WAPEUP_PRIORITY : app_drv_config.h
- app_driver_sem_deinit : app_rtos_cfg.h
- app_driver_sem_init : app_rtos_cfg.h
- app_driver_sem_pend : app_rtos_cfg.h
- app_driver_sem_post : app_rtos_cfg.h
- app_driver_sem_post_from_isr : app_rtos_cfg.h
- APP_DRIVER_SPI_WAPEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_SYSTICK_WAPEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_TIM_WAPEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_UART_WAPEUP_PRIORITY : app_drv_config.h
- APP_DRV_ERR_BUSY : app_drv_error.h
- APP_DRV_ERR_CODE_CHECK : app_drv_error.h
- APP_DRV_ERR_HAL : app_drv_error.h
- APP_DRV_ERR_INVALID_ID : app_drv_error.h
- APP_DRV_ERR_INVALID_MODE : app_drv_error.h
- APP_DRV_ERR_INVALID_PARAM : app_drv_error.h
- APP_DRV_ERR_INVALID_TYPE : app_drv_error.h
- APP_DRV_ERR_POINTER_NULL : app_drv_error.h
- APP_DRV_ERR_TIMEOUT : app_drv_error.h
- APP_DRV_MUTEX_DECL : app_rtos_cfg.h
- APP_DRV_SEM_DECL : app_rtos_cfg.h
- APP_DRV_SUCCESS : app_drv_error.h
- APP_IO_DEFAULT_CONFIG : app_io.h
- APP_IO_PIN_0 : app_io.h
- APP_IO_PIN_1 : app_io.h
- APP_IO_PIN_10 : app_io.h
- APP_IO_PIN_11 : app_io.h
- APP_IO_PIN_12 : app_io.h
- APP_IO_PIN_13 : app_io.h
- APP_IO_PIN_14 : app_io.h
- APP_IO_PIN_15 : app_io.h
- APP_IO_PIN_16 : app_io.h
- APP_IO_PIN_17 : app_io.h
- APP_IO_PIN_18 : app_io.h
- APP_IO_PIN_19 : app_io.h
- APP_IO_PIN_2 : app_io.h
- APP_IO_PIN_20 : app_io.h
- APP_IO_PIN_21 : app_io.h
- APP_IO_PIN_22 : app_io.h
- APP_IO_PIN_23 : app_io.h
- APP_IO_PIN_24 : app_io.h
- APP_IO_PIN_25 : app_io.h
- APP_IO_PIN_26 : app_io.h
- APP_IO_PIN_27 : app_io.h
- APP_IO_PIN_28 : app_io.h
- APP_IO_PIN_29 : app_io.h
- APP_IO_PIN_3 : app_io.h
- APP_IO_PIN_30 : app_io.h
- APP_IO_PIN_31 : app_io.h
- APP_IO_PIN_4 : app_io.h
- APP_IO_PIN_5 : app_io.h
- APP_IO_PIN_6 : app_io.h
- APP_IO_PIN_7 : app_io.h
- APP_IO_PIN_8 : app_io.h
- APP_IO_PIN_9 : app_io.h
- APP_IO_PIN_ALL : app_io.h
- APP_IO_PIN_MASK : app_io.h
- APP_IO_PINS_0_15 : app_io.h
- APP_IO_PINS_16_31 : app_io.h
- APP_MSIO_PIN_ALL : app_io.h
- APP_MSIO_PIN_MASK : app_io.h
- APP_PWM_PIN_DISABLE : app_pwm.h
- APP_PWM_PIN_ENABLE : app_pwm.h
- APP_QSPI_PIN_DISABLE : app_qspi.h
- APP_QSPI_PIN_ENABLE : app_qspi.h
- APP_RTC_ALARM_DISABLE_ALL : app_rtc.h
- APP_RTC_ALARM_DISABLE_DATE : app_rtc.h
- APP_RTC_ALARM_DISABLE_TICK : app_rtc.h
- APP_SLEEP_CB_MAX : app_pwr_mgmt.h
- APP_SPI_PIN_DISABLE : app_spi.h
- APP_SPI_PIN_ENABLE : app_spi.h
- ATT_ENC_KEY_SIZE_16 : ble_gatts.h
- ATT_UUID_TYPE_SET : ble_gatts.h
- ATT_VAL_LOC_STACK : ble_gatts.h
- ATT_VAL_LOC_USER : ble_gatts.h
- AUTH : ble_gatts.h
- AUTH_ALL : ble_sec.h
- AUTH_BOND : ble_sec.h
- AUTH_KEY_PRESS_NOTIFY : ble_sec.h
- AUTH_MITM : ble_sec.h
- AUTH_NONE : ble_sec.h
- AUTH_SEC_CON : ble_sec.h