Macros
QSPI Buad Rate
Peripheral Driver » LL Driver » XQSPI » Defines » XQSPI Exported Constants

## Macros
#define | LL_XQSPI_BAUD_RATE_64M 0x00000000UL
| Clock to 64MHz. More...
#define | LL_XQSPI_BAUD_RATE_48M (1UL << AON_PWR_REG01_XF_SCK_CLK_SEL_Pos)
| Clock to 48MHz. More...
#define | LL_XQSPI_BAUD_RATE_32M (2UL << AON_PWR_REG01_XF_SCK_CLK_SEL_Pos)
| Clock to 32MHz. More...
#define | LL_XQSPI_BAUD_RATE_24M (3UL << AON_PWR_REG01_XF_SCK_CLK_SEL_Pos)
| Clock to 24MHz. More...
#define | LL_XQSPI_BAUD_RATE_16M (4UL << AON_PWR_REG01_XF_SCK_CLK_SEL_Pos)
| Clock to 16MHz. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_XQSPI_BAUD_RATE_16M

#define LL_XQSPI_BAUD_RATE_16M (4UL << AON_PWR_REG01_XF_SCK_CLK_SEL_Pos)

Clock to 16MHz.

Definition at line 283 of file gr55xx_ll_xqspi.h.

## ◆ LL_XQSPI_BAUD_RATE_24M

#define LL_XQSPI_BAUD_RATE_24M (3UL << AON_PWR_REG01_XF_SCK_CLK_SEL_Pos)

Clock to 24MHz.

Definition at line 282 of file gr55xx_ll_xqspi.h.

## ◆ LL_XQSPI_BAUD_RATE_32M

#define LL_XQSPI_BAUD_RATE_32M (2UL << AON_PWR_REG01_XF_SCK_CLK_SEL_Pos)

Clock to 32MHz.

Definition at line 281 of file gr55xx_ll_xqspi.h.

## ◆ LL_XQSPI_BAUD_RATE_48M

#define LL_XQSPI_BAUD_RATE_48M (1UL << AON_PWR_REG01_XF_SCK_CLK_SEL_Pos)

Clock to 48MHz.

Definition at line 280 of file gr55xx_ll_xqspi.h.

## ◆ LL_XQSPI_BAUD_RATE_64M

#define LL_XQSPI_BAUD_RATE_64M 0x00000000UL

Clock to 64MHz.

Definition at line 279 of file gr55xx_ll_xqspi.h.