Functions
Initialization and de-initialization functions
Peripheral Driver » HAL Driver » MSIO » Functions

Initialization and Configuration functions. More...

## Functions
void | hal_msio_init (msio_init_t *p_msio_init)
| Initialize the MSIOx peripheral according to the specified parameters in the msio_init_t. More...
void | hal_msio_deinit (uint32_t msio_pin)
| De-initialize the MSIOx peripheral registers to their default reset values. More...

## Detailed Description

Initialization and Configuration functions.

## Function Documentation

## ◆ hal_msio_deinit()

void hal_msio_deinit | ( | uint32_t | msio_pin | ) |

De-initialize the MSIOx peripheral registers to their default reset values.

Parameters

  [in] | msio_pin | Specifies the port bit to be written. This parameter can be a combination of the following values: MSIO_PIN_0 MSIO_PIN_1 MSIO_PIN_2 MSIO_PIN_3 MSIO_PIN_4 MSIO_PIN_ALL

## ◆ hal_msio_init()

void hal_msio_init | ( | msio_init_t * | p_msio_init | ) |

Initialize the MSIOx peripheral according to the specified parameters in the msio_init_t.

Parameters

  [in] | p_msio_init | Pointer to an msio_init_t structure that contains the configuration information for the specified MSIO peripheral port.