Modules | Macros
Defines
BLE Services » Phone Alert Status Service (PASS)

## Modules
| Characteristics Mask
| Bit masks for the initialization of pass_init_t::char_mask.
| Alert Status BIT
| PASS Alert Status bits.
| Ringer Setting
| The Ringer Setting characteristic defines the setting of the ringer.

## Macros
#define | PASS_CONNECTION_MAX
| Maximum number of Phone Alert Status Service connections. More...
#define | PASS_ALERT_STATUS_VAL_LEN 1
| Length of Alert Status value. More...
#define | PASS_RINGER_SET_VAL_LEN 1
| Length of Ringer Setting value. More...
#define | PASS_RINGER_CTRL_PT_VAL_LEN 1
| Length of Ringer Control Point value. More...

## Detailed Description

## Macro Definition Documentation

## ◆ PASS_ALERT_STATUS_VAL_LEN

#define PASS_ALERT_STATUS_VAL_LEN 1

Length of Alert Status value.

Definition at line 70 of file pass.h.

## ◆ PASS_CONNECTION_MAX

#define PASS_CONNECTION_MAX

Value:
(10 < CFG_MAX_CONNECTIONS ?\
10 : CFG_MAX_CONNECTIONS)

Maximum number of Phone Alert Status Service connections.

Definition at line 69 of file pass.h.

## ◆ PASS_RINGER_CTRL_PT_VAL_LEN

#define PASS_RINGER_CTRL_PT_VAL_LEN 1

Length of Ringer Control Point value.

Definition at line 72 of file pass.h.

## ◆ PASS_RINGER_SET_VAL_LEN

#define PASS_RINGER_SET_VAL_LEN 1

Length of Ringer Setting value.

Definition at line 71 of file pass.h.