Functions
Data_Management
Peripheral Driver » LL Driver » UART » Functions

## Functions
__STATIC_INLINE uint8_t | ll_uart_receive_data8 (uart_regs_t *UARTx)
| Read Receiver Data register (Receive Data value, 8 bits) More...
__STATIC_INLINE void | ll_uart_transmit_data8 (uart_regs_t *UARTx, uint8_t value)
| Write in Transmitter Data Register (Transmit Data value, 8 bits) More...

## Detailed Description

## Function Documentation

## ◆ ll_uart_receive_data8()

__STATIC_INLINE uint8_t ll_uart_receive_data8 | ( | uart_regs_t * | UARTx | ) |

Read Receiver Data register (Receive Data value, 8 bits)

Register | BitsName
--- | ---
RBR | RBR

Parameters

  UARTx | UART instance

Return values

  Value | between Min_Data=0x00 and Max_Data=0xFF

Definition at line 1329 of file gr55xx_ll_uart.h.

## ◆ ll_uart_transmit_data8()

__STATIC_INLINE void ll_uart_transmit_data8 | ( | uart_regs_t * | UARTx,
|  | uint8_t | value
| ) |  |

Write in Transmitter Data Register (Transmit Data value, 8 bits)

Register | BitsName
--- | ---
THR | THR

Parameters

  UARTx | UART instance
  value | between Min_Data=0x00 and Max_Data=0xFF

Return values

  None |

Definition at line 1345 of file gr55xx_ll_uart.h.