### - t -

- THS_C_DOUBLE_MODE : ths_c.h
- THS_C_EVT_DISCOVERY_COMPLETE : ths_c.h
- THS_C_EVT_DISCOVERY_FAIL : ths_c.h
- THS_C_EVT_INVALID : ths_c.h
- THS_C_EVT_PARAM_SET_SUCCESS : ths_c.h
- THS_C_EVT_SETTING_NTF_SET_SUCCESS : ths_c.h
- THS_C_EVT_SETTING_RSP_RECEIVE : ths_c.h
- THS_C_EVT_THRP_DATA_RECEIVE : ths_c.h
- THS_C_EVT_TOGGLE_SET_SUCCESS : ths_c.h
- THS_C_EVT_TX_NTF_SET_SUCCESS : ths_c.h
- THS_C_EVT_TX_SUCCESS : ths_c.h
- THS_C_EVT_WRITE_OP_ERR : ths_c.h
- THS_C_MASTER_WRITE_MODE : ths_c.h
- THS_C_SETTINGS_TYPE_CI : ths_c.h
- THS_C_SETTINGS_TYPE_MTU : ths_c.h
- THS_C_SETTINGS_TYPE_PDU : ths_c.h
- THS_C_SETTINGS_TYPE_PHY : ths_c.h
- THS_C_SETTINGS_TYPE_TRANS_MODE : ths_c.h
- THS_C_SETTINGS_TYPE_TX_POWER : ths_c.h
- THS_C_SLAVE_NOTIFY_MODE : ths_c.h
- THS_DOUBLE_MODE : ths.h
- THS_EVT_DATA_RECEIVED : ths.h
- THS_EVT_DATA_SENT : ths.h
- THS_EVT_INVALID : ths.h
- THS_EVT_SETTINGS_CHANGED : ths.h
- THS_EVT_TOGGLE_SET : ths.h
- THS_MASTER_WRITE_MODE : ths.h
- THS_SETTINGS_TYPE_CI : ths.h
- THS_SETTINGS_TYPE_MTU : ths.h
- THS_SETTINGS_TYPE_PDU : ths.h
- THS_SETTINGS_TYPE_PHY : ths.h
- THS_SETTINGS_TYPE_TRANS_MODE : ths.h
- THS_SETTINGS_TYPE_TX_POWER : ths.h
- THS_SLAVE_NOTIFY_MODE : ths.h
- THS_TOGGLE_STATE_OFF : ths.h
- THS_TOGGLE_STATE_ON : ths.h
- TK_REQ : ble_sec.h
- TPS_C_EVT_DISCOVERY_COMPLETE : tps_c.h
- TPS_C_EVT_DISCOVERY_FAIL : tps_c.h
- TPS_C_EVT_INVALID : tps_c.h
- TPS_C_EVT_TX_POWER_LEVEL_RECEIVE : tps_c.h
- TRC_PWR_ACTIVE_MODE : gr55xx_pwr.h
- TRC_PWR_APP_TIMER_PASS : gr55xx_pwr.h
- TRC_PWR_APP_TIMER_REFUSE : gr55xx_pwr.h
- TRC_PWR_BLE_RET_DSLEEP : gr55xx_pwr.h
- TRC_PWR_BLE_TIMER_PASS : gr55xx_pwr.h
- TRC_PWR_DSLEEP_MODE : gr55xx_pwr.h
- TRC_PWR_WFE_MODE : gr55xx_pwr.h
- TYPE_ADV : ble_gapm.h
- TYPE_INIT : ble_gapm.h
- TYPE_PER_SYNC : ble_gapm.h
- TYPE_SCAN : ble_gapm.h