Functions
Peripheral State and Errors functions
Peripheral Driver » HAL Driver » DMA » Functions

Peripheral State and Errors functions. More...

## Functions
hal_dma_state_t | hal_dma_get_state (dma_handle_t *p_dma)
| Return the DMA hande state. More...
uint32_t | hal_dma_get_error (dma_handle_t *p_dma)
| Return the DMA error code. More...
hal_status_t | hal_dma_suspend_reg (dma_handle_t *p_dma)
| Suspend some registers related to DMA configuration before sleep. More...
hal_status_t | hal_dma_resume_reg (dma_handle_t *p_dma)
| Restore some registers related to DMA configuration after sleep. More...

## Detailed Description

Peripheral State and Errors functions.

     ===============================================================================
                ##### Peripheral State and Errors functions #####
     ===============================================================================
        [..]
        This subsection provides functions allowing to
          (+) Check the DMA state
          (+) Get error code

## Function Documentation

## ◆ hal_dma_get_error()

uint32_t hal_dma_get_error | ( | dma_handle_t * | p_dma | ) |

Return the DMA error code.

Parameters

  [in] | p_dma | Pointer to a DMA handle which contains the configuration information for the specified DMA Channel.

Returns
  DMA Error Code

## ◆ hal_dma_get_state()

hal_dma_state_t hal_dma_get_state | ( | dma_handle_t * | p_dma | ) |

Return the DMA hande state.

Parameters

  [in] | p_dma | Pointer to a DMA handle which contains the configuration information for the specified DMA Channel.

Return values

  HAL_DMA_STATE_RESET | DMA not yet initialized or disabled.
  HAL_DMA_STATE_READY | DMA process succeeded and ready for use.
  HAL_DMA_STATE_BUSY | DMA process is ongoing.
  HAL_DMA_STATE_TIMEOUT | DMA timeout state.
  HAL_DMA_STATE_ERROR | DMA error state.

## ◆ hal_dma_resume_reg()

hal_status_t hal_dma_resume_reg | ( | dma_handle_t * | p_dma | ) |

Restore some registers related to DMA configuration after sleep.

This function must be used in conjunction with the hal_dma_resume_reg().

Parameters

  [in] | p_dma | Pointer to a DMA handle which contains the configuration information for the specified DMA module.

Return values

  HAL_OK | Operation is OK.
  HAL_ERROR | Parameter error or operation not supported.
  HAL_BUSY | Driver is busy.
  HAL_TIMEOUT | Timeout occurred.

## ◆ hal_dma_suspend_reg()

hal_status_t hal_dma_suspend_reg | ( | dma_handle_t * | p_dma | ) |

Suspend some registers related to DMA configuration before sleep.

Parameters

  [in] | p_dma | Pointer to a DMA handle which contains the configuration information for the specified DMA module.

Return values

  HAL_OK | Operation is OK.
  HAL_ERROR | Parameter error or operation not supported.
  HAL_BUSY | Driver is busy.
  HAL_TIMEOUT | Timeout occurred.