Macros
Service and Characteristics UUID
BLE Services » Goodix UART Service Client (GUS_C) » Defines

## Macros
#define | GUS_SVC_UUID
| UUID of GUS Service. More...
#define | GUS_TX_CHAR_UUID
| UUID of GUS Tx characterisitc. More...
#define | GUS_RX_CHAR_UUID
| UUID of GUS Rx characterisitc. More...
#define | GUS_FLOW_CTRL_UUID
| UUID of GUS Flow Control characterisitc. More...
#define | GUS_SVC_UUID
| UUID of GUS Service. More...
#define | GUS_TX_CHAR_UUID
| UUID of GUS Tx characterisitc. More...
#define | GUS_RX_CHAR_UUID
| UUID of GUS Rx characterisitc. More...
#define | GUS_FLOW_CTRL_UUID
| UUID of GUS Flow Control characterisitc. More...

## Detailed Description

## Macro Definition Documentation

## ◆ GUS_FLOW_CTRL_UUID [1/2]

#define GUS_FLOW_CTRL_UUID

Value:
{0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
0x0A, 0x46, 0x44, 0xD3, 0x04, 0x02, 0xED, 0xA6}

UUID of GUS Flow Control characterisitc.

Definition at line 88 of file gus_c.h.

## ◆ GUS_FLOW_CTRL_UUID [2/2]

#define GUS_FLOW_CTRL_UUID

Value:
{0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
0x0A, 0x46, 0x44, 0xD3, 0x04, 0x02, 0xED, 0xA6}

UUID of GUS Flow Control characterisitc.

Definition at line 88 of file mlmr_c.h.

## ◆ GUS_RX_CHAR_UUID [1/2]

#define GUS_RX_CHAR_UUID

Value:
{0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
0x0A, 0x46, 0x44, 0xD3, 0x03, 0x02, 0xED, 0xA6}

UUID of GUS Rx characterisitc.

Definition at line 86 of file gus_c.h.

## ◆ GUS_RX_CHAR_UUID [2/2]

#define GUS_RX_CHAR_UUID

Value:
{0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
0x0A, 0x46, 0x44, 0xD3, 0x03, 0x02, 0xED, 0xA6}

UUID of GUS Rx characterisitc.

Definition at line 86 of file mlmr_c.h.

## ◆ GUS_SVC_UUID [1/2]

#define GUS_SVC_UUID

Value:
{0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
0x0A, 0x46, 0x44, 0xD3, 0x01, 0x02, 0xED, 0xA6}

UUID of GUS Service.

Definition at line 82 of file gus_c.h.

## ◆ GUS_SVC_UUID [2/2]

#define GUS_SVC_UUID

Value:
{0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
0x0A, 0x46, 0x44, 0xD3, 0x01, 0x02, 0xED, 0xA6}

UUID of GUS Service.

Definition at line 82 of file mlmr_c.h.

## ◆ GUS_TX_CHAR_UUID [1/2]

#define GUS_TX_CHAR_UUID

Value:
{0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
0x0A, 0x46, 0x44, 0xD3, 0x02, 0x02, 0xED, 0xA6}

UUID of GUS Tx characterisitc.

Definition at line 84 of file gus_c.h.

## ◆ GUS_TX_CHAR_UUID [2/2]

#define GUS_TX_CHAR_UUID

Value:
{0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
0x0A, 0x46, 0x44, 0xD3, 0x02, 0x02, 0xED, 0xA6}

UUID of GUS Tx characterisitc.

Definition at line 84 of file mlmr_c.h.