Data Fields
thscps_adv_param_t Struct Reference
BLE Services » Throughput Control Point Client (THSCPS) » Structures

THS Control Point Advertising Parameters. More...

`#include <thscps.h>`

## Data Fields
thscps_adv_phy_t | phy
uint16_t | interval
uint16_t | duration
int8_t | tx_power

## Detailed Description

THS Control Point Advertising Parameters.

## Field Documentation

## ◆ duration

uint16_t thscps_adv_param_t::duration

Advertising duration.

## ◆ interval

uint16_t thscps_adv_param_t::interval

Advertising interval.

## ◆ phy

thscps_adv_phy_t thscps_adv_param_t::phy

Specify what PHY the Controller has changed for TX/RX.

## ◆ tx_power

int8_t thscps_adv_param_t::tx_power

Advertising tx power.

The documentation for this struct was generated from the following file:

- thscps.h