Macros
QSPI Datawidth
Peripheral Driver » LL Driver » XQSPI » Defines » XQSPI Exported Constants

## Macros
#define | LL_XQSPI_QSPI_DATASIZE_4BIT 0x00000000UL
| Data length for XQSPI transfer: 4 bits. More...
#define | LL_XQSPI_QSPI_DATASIZE_8BIT (1UL << XQSPI_QSPI_AUXCTRL_BITSIZE_Pos)
| Data length for XQSPI transfer: 8 bits. More...
#define | LL_XQSPI_QSPI_DATASIZE_12BIT (2UL << XQSPI_QSPI_AUXCTRL_BITSIZE_Pos)
| Data length for XQSPI transfer: 12 bits. More...
#define | LL_XQSPI_QSPI_DATASIZE_16BIT (3UL << XQSPI_QSPI_AUXCTRL_BITSIZE_Pos)
| Data length for XQSPI transfer: 16 bits. More...
#define | LL_XQSPI_QSPI_DATASIZE_20BIT (4UL << XQSPI_QSPI_AUXCTRL_BITSIZE_Pos)
| Data length for XQSPI transfer: 20 bits. More...
#define | LL_XQSPI_QSPI_DATASIZE_24BIT (5UL << XQSPI_QSPI_AUXCTRL_BITSIZE_Pos)
| Data length for XQSPI transfer: 24 bits. More...
#define | LL_XQSPI_QSPI_DATASIZE_28BIT (6UL << XQSPI_QSPI_AUXCTRL_BITSIZE_Pos)
| Data length for XQSPI transfer: 28 bits. More...
#define | LL_XQSPI_QSPI_DATASIZE_32BIT (7UL << XQSPI_QSPI_AUXCTRL_BITSIZE_Pos)
| Data length for XQSPI transfer: 32 bits. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_XQSPI_QSPI_DATASIZE_12BIT

#define LL_XQSPI_QSPI_DATASIZE_12BIT (2UL << XQSPI_QSPI_AUXCTRL_BITSIZE_Pos)

Data length for XQSPI transfer: 12 bits.

Definition at line 254 of file gr55xx_ll_xqspi.h.

## ◆ LL_XQSPI_QSPI_DATASIZE_16BIT

#define LL_XQSPI_QSPI_DATASIZE_16BIT (3UL << XQSPI_QSPI_AUXCTRL_BITSIZE_Pos)

Data length for XQSPI transfer: 16 bits.

Definition at line 255 of file gr55xx_ll_xqspi.h.

## ◆ LL_XQSPI_QSPI_DATASIZE_20BIT

#define LL_XQSPI_QSPI_DATASIZE_20BIT (4UL << XQSPI_QSPI_AUXCTRL_BITSIZE_Pos)

Data length for XQSPI transfer: 20 bits.

Definition at line 256 of file gr55xx_ll_xqspi.h.

## ◆ LL_XQSPI_QSPI_DATASIZE_24BIT

#define LL_XQSPI_QSPI_DATASIZE_24BIT (5UL << XQSPI_QSPI_AUXCTRL_BITSIZE_Pos)

Data length for XQSPI transfer: 24 bits.

Definition at line 257 of file gr55xx_ll_xqspi.h.

## ◆ LL_XQSPI_QSPI_DATASIZE_28BIT

#define LL_XQSPI_QSPI_DATASIZE_28BIT (6UL << XQSPI_QSPI_AUXCTRL_BITSIZE_Pos)

Data length for XQSPI transfer: 28 bits.

Definition at line 258 of file gr55xx_ll_xqspi.h.

## ◆ LL_XQSPI_QSPI_DATASIZE_32BIT

#define LL_XQSPI_QSPI_DATASIZE_32BIT (7UL << XQSPI_QSPI_AUXCTRL_BITSIZE_Pos)

Data length for XQSPI transfer: 32 bits.

Definition at line 259 of file gr55xx_ll_xqspi.h.

## ◆ LL_XQSPI_QSPI_DATASIZE_4BIT

#define LL_XQSPI_QSPI_DATASIZE_4BIT 0x00000000UL

Data length for XQSPI transfer: 4 bits.

Definition at line 252 of file gr55xx_ll_xqspi.h.

## ◆ LL_XQSPI_QSPI_DATASIZE_8BIT

#define LL_XQSPI_QSPI_DATASIZE_8BIT (1UL << XQSPI_QSPI_AUXCTRL_BITSIZE_Pos)

Data length for XQSPI transfer: 8 bits.

Definition at line 253 of file gr55xx_ll_xqspi.h.