Macros
InitStruct default configuartion
Peripheral Driver » LL Driver » AON_GPIO » Defines » AON_GPIO Private Macros

## Macros
#define | LL_AON_GPIO_DEFAULT_CONFIG
| LL AON_GPIO InitStrcut default configuartion. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_AON_GPIO_DEFAULT_CONFIG

#define LL_AON_GPIO_DEFAULT_CONFIG

Value:
{ \
.pin = LL_AON_GPIO_PIN_ALL, \
.mode = LL_AON_GPIO_MODE_INPUT, \
.pull = LL_AON_GPIO_PULL_DOWN, \
.mux = LL_AON_GPIO_MUX_7, \
.trigger = LL_AON_GPIO_TRIGGER_NONE, \
}

LL AON_GPIO InitStrcut default configuartion.

Definition at line 233 of file gr55xx_ll_aon_gpio.h.

LL_AON_GPIO_PIN_ALL
#define LL_AON_GPIO_PIN_ALL
Select all pins.
Definition: gr55xx_ll_aon_gpio.h:126
LL_AON_GPIO_TRIGGER_NONE
#define LL_AON_GPIO_TRIGGER_NONE
No Trigger Mode.
Definition: gr55xx_ll_aon_gpio.h:163
LL_AON_GPIO_PULL_DOWN
#define LL_AON_GPIO_PULL_DOWN
Select I/O pull down.
Definition: gr55xx_ll_aon_gpio.h:142
LL_AON_GPIO_MODE_INPUT
#define LL_AON_GPIO_MODE_INPUT
Select input mode.
Definition: gr55xx_ll_aon_gpio.h:132
LL_AON_GPIO_MUX_7
#define LL_AON_GPIO_MUX_7
Definition: gr55xx_ll_aon_gpio.h:155