Functions
Initialization and de-initialization functions
Peripheral Driver » LL Driver » MSIO » Functions

## Functions
error_status_t | ll_msio_deinit (void)
| De-initialize MSIO registers (Registers restored to their default values). More...
error_status_t | ll_msio_init (ll_msio_init_t *p_msio_init)
| Initialize MSIO registers according to the specified. More...
void | ll_msio_struct_init (ll_msio_init_t *p_msio_init)
| Set each field of a ll_msio_init_t type structure to default value. More...

## Detailed Description

## Function Documentation

## ◆ ll_msio_deinit()

error_status_t ll_msio_deinit | ( | void |  | ) |

De-initialize MSIO registers (Registers restored to their default values).

Return values

  An | error_status_t enumeration value: SUCCESS: MSIO registers are de-initialized ERROR: MSIO registers are not de-initialized

## ◆ ll_msio_init()

error_status_t ll_msio_init | ( | ll_msio_init_t * | p_msio_init | ) |

Initialize MSIO registers according to the specified.

parameters in p_msio_init.

Parameters

  p_msio_init | Pointer to a ll_msio_init_t structure that contains the configuration information for the specified MSIO peripheral.

Return values

  An | error_status_t enumeration value: SUCCESS: MSIO registers are initialized according to p_msio_init content ERROR: Problem occurred during MSIO Registers initialization

## ◆ ll_msio_struct_init()

void ll_msio_struct_init | ( | ll_msio_init_t * | p_msio_init | ) |

Set each field of a ll_msio_init_t type structure to default value.

Parameters

  p_msio_init | Pointer to a ll_msio_init_t structure whose fields will be set to default values.

Return values

  None |