Modules | Macros
Defines
BLE Services » Device Information Service (DIS)

## Modules
| Characteristics Mask
| Bit masks for the initialization of dis_init_t::char_mask.
| IEEE 11073-20601 Authoritative Body Type

## Macros
#define | DIS_CONNECTION_MAX
| Maximum number of DIS connections. More...
#define | DIS_SYS_ID_LEN 8
| System ID length. More...
#define | DIS_PNP_ID_LEN 7
| PnP ID length. More...
#define | DIS_VAL_MAX_LEN 128
| Maximal length for Characteristic values - 128 bytes. More...
#define | DIS_IEEE_CERTIF_MIN_LEN 6
| IEEE Certification length (min 6 bytes). More...

## Detailed Description

## Macro Definition Documentation

## ◆ DIS_CONNECTION_MAX

#define DIS_CONNECTION_MAX

Value:
(10 < CFG_MAX_CONNECTIONS ?\
10 : CFG_MAX_CONNECTIONS)

Maximum number of DIS connections.

The value is configurable.

Definition at line 75 of file dis.h.

## ◆ DIS_IEEE_CERTIF_MIN_LEN

#define DIS_IEEE_CERTIF_MIN_LEN 6

IEEE Certification length (min 6 bytes).

Definition at line 79 of file dis.h.

## ◆ DIS_PNP_ID_LEN

#define DIS_PNP_ID_LEN 7

PnP ID length.

Definition at line 77 of file dis.h.

## ◆ DIS_SYS_ID_LEN

#define DIS_SYS_ID_LEN 8

System ID length.

Definition at line 76 of file dis.h.

## ◆ DIS_VAL_MAX_LEN

#define DIS_VAL_MAX_LEN 128

Maximal length for Characteristic values - 128 bytes.

Definition at line 78 of file dis.h.