Macros
Datawidth
Peripheral Driver » LL Driver » SPI » Defines » SPI Exported Constants

## Macros
#define | LL_SSI_DATASIZE_4BIT (3UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 4 bits. More...
#define | LL_SSI_DATASIZE_5BIT (4UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 5 bits. More...
#define | LL_SSI_DATASIZE_6BIT (5UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 6 bits. More...
#define | LL_SSI_DATASIZE_7BIT (6UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 7 bits. More...
#define | LL_SSI_DATASIZE_8BIT (7UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 8 bits. More...
#define | LL_SSI_DATASIZE_9BIT (8UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 9 bits. More...
#define | LL_SSI_DATASIZE_10BIT (9UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 10 bits. More...
#define | LL_SSI_DATASIZE_11BIT (10UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 11 bits. More...
#define | LL_SSI_DATASIZE_12BIT (11UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 12 bits. More...
#define | LL_SSI_DATASIZE_13BIT (12UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 13 bits. More...
#define | LL_SSI_DATASIZE_14BIT (13UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 14 bits. More...
#define | LL_SSI_DATASIZE_15BIT (14UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 15 bits. More...
#define | LL_SSI_DATASIZE_16BIT (15UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 16 bits. More...
#define | LL_SSI_DATASIZE_17BIT (16UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 17 bits. More...
#define | LL_SSI_DATASIZE_18BIT (17UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 18 bits. More...
#define | LL_SSI_DATASIZE_19BIT (18UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 19 bits. More...
#define | LL_SSI_DATASIZE_20BIT (19UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 20 bits. More...
#define | LL_SSI_DATASIZE_21BIT (20UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 21 bits. More...
#define | LL_SSI_DATASIZE_22BIT (21UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 22 bits. More...
#define | LL_SSI_DATASIZE_23BIT (22UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 23 bits. More...
#define | LL_SSI_DATASIZE_24BIT (23UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 24 bits. More...
#define | LL_SSI_DATASIZE_25BIT (24UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 25 bits. More...
#define | LL_SSI_DATASIZE_26BIT (25UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 26 bits. More...
#define | LL_SSI_DATASIZE_27BIT (26UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 27 bits. More...
#define | LL_SSI_DATASIZE_28BIT (27UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 28 bits. More...
#define | LL_SSI_DATASIZE_29BIT (28UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 29 bits. More...
#define | LL_SSI_DATASIZE_30BIT (29UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 30 bits. More...
#define | LL_SSI_DATASIZE_31BIT (30UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 31 bits. More...
#define | LL_SSI_DATASIZE_32BIT (31UL << SSI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 32 bits. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_SSI_DATASIZE_10BIT

#define LL_SSI_DATASIZE_10BIT (9UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 10 bits.

Definition at line 257 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_11BIT

#define LL_SSI_DATASIZE_11BIT (10UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 11 bits.

Definition at line 258 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_12BIT

#define LL_SSI_DATASIZE_12BIT (11UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 12 bits.

Definition at line 259 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_13BIT

#define LL_SSI_DATASIZE_13BIT (12UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 13 bits.

Definition at line 260 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_14BIT

#define LL_SSI_DATASIZE_14BIT (13UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 14 bits.

Definition at line 261 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_15BIT

#define LL_SSI_DATASIZE_15BIT (14UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 15 bits.

Definition at line 262 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_16BIT

#define LL_SSI_DATASIZE_16BIT (15UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 16 bits.

Definition at line 263 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_17BIT

#define LL_SSI_DATASIZE_17BIT (16UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 17 bits.

Definition at line 264 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_18BIT

#define LL_SSI_DATASIZE_18BIT (17UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 18 bits.

Definition at line 265 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_19BIT

#define LL_SSI_DATASIZE_19BIT (18UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 19 bits.

Definition at line 266 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_20BIT

#define LL_SSI_DATASIZE_20BIT (19UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 20 bits.

Definition at line 267 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_21BIT

#define LL_SSI_DATASIZE_21BIT (20UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 21 bits.

Definition at line 268 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_22BIT

#define LL_SSI_DATASIZE_22BIT (21UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 22 bits.

Definition at line 269 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_23BIT

#define LL_SSI_DATASIZE_23BIT (22UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 23 bits.

Definition at line 270 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_24BIT

#define LL_SSI_DATASIZE_24BIT (23UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 24 bits.

Definition at line 271 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_25BIT

#define LL_SSI_DATASIZE_25BIT (24UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 25 bits.

Definition at line 272 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_26BIT

#define LL_SSI_DATASIZE_26BIT (25UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 26 bits.

Definition at line 273 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_27BIT

#define LL_SSI_DATASIZE_27BIT (26UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 27 bits.

Definition at line 274 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_28BIT

#define LL_SSI_DATASIZE_28BIT (27UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 28 bits.

Definition at line 275 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_29BIT

#define LL_SSI_DATASIZE_29BIT (28UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 29 bits.

Definition at line 276 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_30BIT

#define LL_SSI_DATASIZE_30BIT (29UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 30 bits.

Definition at line 277 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_31BIT

#define LL_SSI_DATASIZE_31BIT (30UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 31 bits.

Definition at line 278 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_32BIT

#define LL_SSI_DATASIZE_32BIT (31UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 32 bits.

Definition at line 279 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_4BIT

#define LL_SSI_DATASIZE_4BIT (3UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 4 bits.

Definition at line 251 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_5BIT

#define LL_SSI_DATASIZE_5BIT (4UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 5 bits.

Definition at line 252 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_6BIT

#define LL_SSI_DATASIZE_6BIT (5UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 6 bits.

Definition at line 253 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_7BIT

#define LL_SSI_DATASIZE_7BIT (6UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 7 bits.

Definition at line 254 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_8BIT

#define LL_SSI_DATASIZE_8BIT (7UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 8 bits.

Definition at line 255 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_DATASIZE_9BIT

#define LL_SSI_DATASIZE_9BIT (8UL << SSI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 9 bits.

Definition at line 256 of file gr55xx_ll_spi.h.