### - m -

- major : sdk_version_t
- manuf_name : ble_gap_dev_version_ind_t
- map : ble_gap_chnl_map_t
- master_ack_count : _i2c_handle
- max_adv_data_len : ble_gap_dev_info_t
- max_adv_evt : ble_gap_adv_time_param_t
- max_data_len : ble_gap_dev_info_t
- max_nb_attr : ble_gatts_create_db_t
- max_rx_octets : ble_gap_evt_data_length_t
- max_rx_time : ble_gap_evt_data_length_t
- max_size : ble_gatts_attm_desc_128_t , ble_gatts_attm_desc_t
- max_skip : ble_gap_adv_second_cfg_t
- max_tx_octets : ble_gap_evt_data_length_t
- max_tx_pwr : ble_gap_adv_param_t , ble_gap_dev_tx_power_t , ble_gap_ext_adv_param_t
- max_tx_time : ble_gap_evt_data_length_t
- min : _calendar_alarm , _calendar_time
- min_tx_pwr : ble_gap_dev_tx_power_t
- minor : sdk_version_t
- miso : app_spi_pin_cfg_t
- mks_flag : ble_gap_lepsm_register_t
- mode : _aon_gpio_init , _calendar_handle , _dma_init , _gpio_init , _hmac_init , _i2c_handle , _ll_aon_gpio_init , _ll_dma_init , _ll_gpio_init , _ll_msio_init , _ll_pwm_init_t , _ll_xqspi_init_t , _msio_init , app_gpiote_param_t , app_io_init_t , app_qspi_pin_t , app_spi_pin_t , gdx_lcp_config_t , pwm_init_t
- mon : _calendar_time
- mosi : app_spi_pin_cfg_t
- mps : ble_l2cap_lecb_cfm_conn_t , ble_l2cap_lecb_conn_req_t
- ms : _calendar_handle , _calendar_time
- msg_ret : stack_heaps_table_t
- msg_ret_size : stack_heaps_table_t
- msp_deinit : _hal_callback
- msp_init : _hal_callback
- mtu : ble_gatt_common_evt_mtu_exchange_t , ble_l2cap_lecb_cfm_conn_t , ble_l2cap_lecb_conn_req_t
- mtu_exchange : ble_gatt_common_evt_t
- multi_channel : adc_env_t
- mux : _aon_gpio_init , _gpio_init , _ll_aon_gpio_init , _ll_gpio_init , _ll_msio_init , _msio_init , app_adc_pin_t , app_comp_pin_t , app_i2c_pin_t , app_i2s_pin_t , app_io_init_t , app_iso7816_pin_t , app_pwm_pin_t , app_qspi_pin_t , app_spi_pin_t , app_uart_pin_t