Public Attributes | List of all members
app_spi_pin_t Struct Reference
Peripheral Driver » APP DRIVER » SPI » Structures

SPI IO Structures. More...

`#include <app_spi.h>`

## Public Attributes
app_io_type_t | type
| Specifies the type of SPI IO. More...
app_io_mux_t | mux
| Specifies the Peripheral to be connected to the selected pins. More...
uint32_t | pin
| Specifies the IO pins to be configured. More...
app_io_mode_t | mode
| Specifies the mode for the selected pins. More...
app_io_pull_t | pull
| Specifies the Pull-up or Pull-Down activation for the selected pins. More...
uint8_t | enable
| Enable or disable the pin. More...

## Detailed Description

SPI IO Structures.

Definition at line 109 of file app_spi.h.

## Member Data Documentation

## ◆ enable

uint8_t app_spi_pin_t::enable

Enable or disable the pin.

Definition at line 117 of file app_spi.h.

## ◆ mode

app_io_mode_t app_spi_pin_t::mode

Specifies the mode for the selected pins.

Definition at line 115 of file app_spi.h.

## ◆ mux

app_io_mux_t app_spi_pin_t::mux

Specifies the Peripheral to be connected to the selected pins.

Definition at line 112 of file app_spi.h.

## ◆ pin

uint32_t app_spi_pin_t::pin

Specifies the IO pins to be configured.

This parameter can be any value of Defines.

Definition at line 113 of file app_spi.h.

## ◆ pull

app_io_pull_t app_spi_pin_t::pull

Specifies the Pull-up or Pull-Down activation for the selected pins.

Definition at line 116 of file app_spi.h.

## ◆ type

app_io_type_t app_spi_pin_t::type

Specifies the type of SPI IO.

Definition at line 111 of file app_spi.h.

The documentation for this struct was generated from the following file:

- app_spi.h