### - f -

- features : ble_gap_peer_features_ind_t
- filter_pol : ble_gap_adv_param_t , ble_gap_ext_adv_param_t
- finish_transfers : hci_uart_call_t
- flash_id : _exflash_handle
- flash_size : _exflash_handle
- flow_off : hci_uart_call_t
- flow_on : hci_uart_call_t
- force_clk : _cgc_init
- force_clk0 : _ll_cgc_init_t
- force_clk1 : _ll_cgc_init_t
- force_clk2 : _ll_cgc_init_t
- freq : gdx_lcp_config_t , pwm_init_t
- fw_mode : _exflash_handle