Macros
QSPI Interrupts
Peripheral Driver » HAL Driver » QSPI » Defines » QSPI Exported Constants
Collaboration diagram for QSPI Interrupts:

## Macros
#define | QSPI_IT_MST LL_SSI_IS_MST
| Multi-Master Contention Interrupt flag. More...
#define | QSPI_IT_RXF LL_SSI_IS_RXF
| Receive FIFO Full Interrupt flag More...
#define | QSPI_IT_RXO LL_SSI_IS_RXO
| Receive FIFO Overflow Interrupt flag More...
#define | QSPI_IT_RXU LL_SSI_IS_RXU
| Receive FIFO Underflow Interrupt flag More...
#define | QSPI_IT_TXO LL_SSI_IS_TXO
| Transmit FIFO Overflow Interrupt flag More...
#define | QSPI_IT_TXE LL_SSI_IS_TXE
| Transmit FIFO Empty Interrupt flag More...

## Detailed Description

## Macro Definition Documentation

## ◆ QSPI_IT_MST

#define QSPI_IT_MST LL_SSI_IS_MST

Multi-Master Contention Interrupt flag.

Definition at line 350 of file gr55xx_hal_qspi.h.

## ◆ QSPI_IT_RXF

#define QSPI_IT_RXF LL_SSI_IS_RXF

Receive FIFO Full Interrupt flag

Definition at line 351 of file gr55xx_hal_qspi.h.

## ◆ QSPI_IT_RXO

#define QSPI_IT_RXO LL_SSI_IS_RXO

Receive FIFO Overflow Interrupt flag

Definition at line 352 of file gr55xx_hal_qspi.h.

## ◆ QSPI_IT_RXU

#define QSPI_IT_RXU LL_SSI_IS_RXU

Receive FIFO Underflow Interrupt flag

Definition at line 353 of file gr55xx_hal_qspi.h.

## ◆ QSPI_IT_TXE

#define QSPI_IT_TXE LL_SSI_IS_TXE

Transmit FIFO Empty Interrupt flag

Definition at line 355 of file gr55xx_hal_qspi.h.

## ◆ QSPI_IT_TXO

#define QSPI_IT_TXO LL_SSI_IS_TXO

Transmit FIFO Overflow Interrupt flag

Definition at line 354 of file gr55xx_hal_qspi.h.