Public Attributes | List of all members
ble_gap_max_adv_data_len_ind_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

Maximum advertising data length info. More...

`#include <ble_gapc.h>`

## Public Attributes
uint16_t | length
| Maximum advertising data length supported by controller. More...

## Detailed Description

Maximum advertising data length info.

Definition at line 230 of file ble_gapc.h.

## Member Data Documentation

## ◆ length

uint16_t ble_gap_max_adv_data_len_ind_t::length

Maximum advertising data length supported by controller.

Definition at line 232 of file ble_gapc.h.

The documentation for this struct was generated from the following file:

- ble_gapc.h