Public Attributes | List of all members
app_io_init_t Struct Reference
Peripheral Driver » APP DRIVER » GPIO » Defines » Structures

GPIO parameter structure definition. More...

`#include <app_io.h>`

## Public Attributes
uint32_t | pin
| Specifies the IO pins to be configured. More...
app_io_mode_t | mode
| Specifies the operating mode for the selected pins. More...
app_io_pull_t | pull
| Specifies the Pull-up or Pull-Down activation for the selected pins. More...
app_io_mux_t | mux
| Specifies the Peripheral to be connected to the selected pins. More...

## Detailed Description

GPIO parameter structure definition.

Definition at line 286 of file app_io.h.

## Member Data Documentation

## ◆ mode

app_io_mode_t app_io_init_t::mode

Specifies the operating mode for the selected pins.

Definition at line 290 of file app_io.h.

## ◆ mux

app_io_mux_t app_io_init_t::mux

Specifies the Peripheral to be connected to the selected pins.

Definition at line 292 of file app_io.h.

## ◆ pin

uint32_t app_io_init_t::pin

Specifies the IO pins to be configured.

This parameter can be any value of Defines

Definition at line 288 of file app_io.h.

## ◆ pull

app_io_pull_t app_io_init_t::pull

Specifies the Pull-up or Pull-Down activation for the selected pins.

Definition at line 291 of file app_io.h.

The documentation for this struct was generated from the following file:

- app_io.h