### - a -

- AON_GPIO_PIN_RESET : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_SET : gr55xx_hal_aon_gpio.h
- APP_ADC_ACTIVITY : app_adc.h
- APP_ADC_DMA_ACTIVITY : app_adc.h
- APP_ADC_DMA_INVALID : app_adc.h
- APP_ADC_EVT_CONV_CPLT : app_adc.h
- APP_ADC_INVALID : app_adc.h
- APP_AES_ACTIVITY : app_aes.h
- APP_AES_EVT_DONE : app_aes.h
- APP_AES_EVT_ERROR : app_aes.h
- APP_AES_INVALID : app_aes.h
- APP_AES_MODE_CBC : app_aes.h
- APP_AES_MODE_ECB : app_aes.h
- APP_AES_MODE_MAX : app_aes.h
- APP_AON_WDT_ACTIVITY : app_aon_wdt.h
- APP_AON_WDT_INVALID : app_aon_wdt.h
- APP_COMP_ACTIVITY : app_comp.h
- APP_COMP_EVT_DONE : app_comp.h
- APP_COMP_EVT_ERROR : app_comp.h
- APP_COMP_INVALID : app_comp.h
- APP_DMA_ACTIVITY : app_dma.h
- APP_DMA_EVT_BLK : app_dma.h
- APP_DMA_EVT_ERROR : app_dma.h
- APP_DMA_EVT_TFR : app_dma.h
- APP_DMA_INVALID : app_dma.h
- APP_DUAL_TIM_ACTIVITY : app_dual_tim.h
- APP_DUAL_TIM_EVT_DONE : app_dual_tim.h
- APP_DUAL_TIM_EVT_ERROR : app_dual_tim.h
- APP_DUAL_TIM_ID_0 : app_dual_tim.h
- APP_DUAL_TIM_ID_1 : app_dual_tim.h
- APP_DUAL_TIM_ID_MAX : app_dual_tim.h
- APP_DUAL_TIM_INVALID : app_dual_tim.h
- APP_HMAC_ACTIVITY : app_hmac.h
- APP_HMAC_EVT_DONE : app_hmac.h
- APP_HMAC_EVT_ERROR : app_hmac.h
- APP_HMAC_INVALID : app_hmac.h
- APP_HMAC_TYPE_DMA : app_hmac.h
- APP_HMAC_TYPE_INTERRUPT : app_hmac.h
- APP_HMAC_TYPE_MAX : app_hmac.h
- APP_HMAC_TYPE_POLLING : app_hmac.h
- APP_I2C_ABORT : app_i2c.h
- APP_I2C_ACTIVITY : app_i2c.h
- APP_I2C_DMA_ACTIVITY : app_i2c.h
- APP_I2C_DMA_INVALID : app_i2c.h
- APP_I2C_EVT_ERROR : app_i2c.h
- APP_I2C_EVT_RX_DATA : app_i2c.h
- APP_I2C_EVT_TX_CPLT : app_i2c.h
- APP_I2C_ID_0 : app_i2c.h
- APP_I2C_ID_1 : app_i2c.h
- APP_I2C_ID_MAX : app_i2c.h
- APP_I2C_INVALID : app_i2c.h
- APP_I2C_ROLE_MASTER : app_i2c.h
- APP_I2C_ROLE_MAX : app_i2c.h
- APP_I2C_ROLE_SLAVE : app_i2c.h
- APP_I2S_ACTIVITY : app_i2s.h
- APP_I2S_DMA_ACTIVITY : app_i2s.h
- APP_I2S_DMA_INVALID : app_i2s.h
- APP_I2S_EVT_ERROR : app_i2s.h
- APP_I2S_EVT_RX_DATA : app_i2s.h
- APP_I2S_EVT_TX_CPLT : app_i2s.h
- APP_I2S_EVT_TX_RX : app_i2s.h
- APP_I2S_ID_MASTER : app_i2s.h
- APP_I2S_ID_MAX : app_i2s.h
- APP_I2S_ID_SLAVE : app_i2s.h
- APP_I2S_INVALID : app_i2s.h
- APP_IO_INPUT_TYPE_CMOS : app_io.h
- APP_IO_INPUT_TYPE_MAX : app_io.h
- APP_IO_INPUT_TYPE_SCHMITT : app_io.h
- APP_IO_MODE_ANALOG : app_io.h
- APP_IO_MODE_INPUT : app_io.h
- APP_IO_MODE_IT_FALLING : app_io.h
- APP_IO_MODE_IT_HIGH : app_io.h
- APP_IO_MODE_IT_LOW : app_io.h
- APP_IO_MODE_IT_RISING : app_io.h
- APP_IO_MODE_MAX : app_io.h
- APP_IO_MODE_MUX : app_io.h
- APP_IO_MODE_NONE : app_io.h
- APP_IO_MODE_OUTPUT : app_io.h
- APP_IO_MUX_0 : app_io.h
- APP_IO_MUX_1 : app_io.h
- APP_IO_MUX_2 : app_io.h
- APP_IO_MUX_3 : app_io.h
- APP_IO_MUX_4 : app_io.h
- APP_IO_MUX_5 : app_io.h
- APP_IO_MUX_6 : app_io.h
- APP_IO_MUX_7 : app_io.h
- APP_IO_MUX_8 : app_io.h
- APP_IO_MUX_MAX : app_io.h
- APP_IO_NOPULL : app_io.h
- APP_IO_PIN_RESET : app_io.h
- APP_IO_PIN_SET : app_io.h
- APP_IO_PULL_MAX : app_io.h
- APP_IO_PULLDOWN : app_io.h
- APP_IO_PULLUP : app_io.h
- APP_IO_SPPED_HIGH : app_io.h
- APP_IO_SPPED_MAX : app_io.h
- APP_IO_SPPED_MEDIUM : app_io.h
- APP_IO_STRENGTH_HIGH : app_io.h
- APP_IO_STRENGTH_LOW : app_io.h
- APP_IO_STRENGTH_MAX : app_io.h
- APP_IO_STRENGTH_MEDIUM : app_io.h
- APP_IO_STRENGTH_ULTRA : app_io.h
- APP_IO_TYPE_AON : app_io.h
- APP_IO_TYPE_GPIOA : app_io.h
- APP_IO_TYPE_GPIOB : app_io.h
- APP_IO_TYPE_GPIOC : app_io.h
- APP_IO_TYPE_MAX : app_io.h
- APP_IO_TYPE_MSIO : app_io.h
- APP_IO_TYPE_NORMAL : app_io.h
- APP_ISO7816_ACTIVITY : app_iso7816.h
- APP_ISO7816_EVT_ABORT : app_iso7816.h
- APP_ISO7816_EVT_ATR_CPLT : app_iso7816.h
- APP_ISO7816_EVT_ERROR : app_iso7816.h
- APP_ISO7816_EVT_PRESENCE : app_iso7816.h
- APP_ISO7816_EVT_RX_CPLT : app_iso7816.h
- APP_ISO7816_EVT_TX_CPLT : app_iso7816.h
- APP_ISO7816_EVT_TX_RX_CPLT : app_iso7816.h
- APP_ISO7816_INVALID : app_iso7816.h
- APP_ISO7816_TYPE_INTERRUPT : app_iso7816.h
- APP_ISO7816_TYPE_MAX : app_iso7816.h
- APP_ISO7816_TYPE_POLLING : app_iso7816.h
- APP_PKC_ACTIVITY : app_pkc.h
- APP_PKC_EVT_DONE : app_pkc.h
- APP_PKC_EVT_ERROR : app_pkc.h
- APP_PKC_INVALID : app_pkc.h
- APP_PKC_TYPE_INTERRUPT : app_pkc.h
- APP_PKC_TYPE_MAX : app_pkc.h
- APP_PKC_TYPE_POLLING : app_pkc.h
- APP_PWM_ACTIVE_CHANNEL_A : app_pwm.h
- APP_PWM_ACTIVE_CHANNEL_ALL : app_pwm.h
- APP_PWM_ACTIVE_CHANNEL_B : app_pwm.h
- APP_PWM_ACTIVE_CHANNEL_C : app_pwm.h
- APP_PWM_ACTIVE_CHANNEL_CLEARED : app_pwm.h
- APP_PWM_ACTIVITY : app_pwm.h
- APP_PWM_ID_0 : app_pwm.h
- APP_PWM_ID_1 : app_pwm.h
- APP_PWM_ID_MAX : app_pwm.h
- APP_PWM_INVALID : app_pwm.h
- APP_PWM_START : app_pwm.h
- APP_PWM_STOP : app_pwm.h
- APP_QSPI_ACTIVITY : app_qspi.h
- APP_QSPI_DMA_ACTIVITY : app_qspi.h
- APP_QSPI_DMA_INVALID : app_qspi.h
- APP_QSPI_EVT_ABORT : app_qspi.h
- APP_QSPI_EVT_ERROR : app_qspi.h
- APP_QSPI_EVT_RX_DATA : app_qspi.h
- APP_QSPI_EVT_TX_CPLT : app_qspi.h
- APP_QSPI_ID_0 : app_qspi.h
- APP_QSPI_ID_1 : app_qspi.h
- APP_QSPI_ID_MAX : app_qspi.h
- APP_QSPI_INVALID : app_qspi.h
- APP_RNG_ACTIVITY : app_rng.h
- APP_RNG_EVT_DONE : app_rng.h
- APP_RNG_EVT_ERROR : app_rng.h
- APP_RNG_INVALID : app_rng.h
- APP_RNG_TYPE_INTERRUPT : app_rng.h
- APP_RNG_TYPE_MAX : app_rng.h
- APP_RNG_TYPE_POLLING : app_rng.h
- APP_RTC_EVT_DATE_ALARM : app_rtc.h
- APP_RTC_EVT_OVERFLOW : app_rtc.h
- APP_RTC_EVT_TICK_ALARM : app_rtc.h
- APP_SPI_ACTIVITY : app_spi.h
- APP_SPI_DMA_ACTIVITY : app_spi.h
- APP_SPI_DMA_INVALID : app_spi.h
- APP_SPI_EVT_ABORT : app_spi.h
- APP_SPI_EVT_ERROR : app_spi.h
- APP_SPI_EVT_RX_CPLT : app_spi.h
- APP_SPI_EVT_TX_CPLT : app_spi.h
- APP_SPI_EVT_TX_RX_CPLT : app_spi.h
- APP_SPI_ID_MASTER : app_spi.h
- APP_SPI_ID_MAX : app_spi.h
- APP_SPI_ID_SLAVE : app_spi.h
- APP_SPI_INVALID : app_spi.h
- APP_TIM_ACTIVITY : app_tim.h
- APP_TIM_EVT_DONE : app_tim.h
- APP_TIM_EVT_ERROR : app_tim.h
- APP_TIM_ID_0 : app_tim.h
- APP_TIM_ID_1 : app_tim.h
- APP_TIM_ID_MAX : app_tim.h
- APP_TIM_INVALID : app_tim.h
- APP_UART_ACTIVITY : app_uart.h
- APP_UART_DMA_ACTIVITY : app_uart.h
- APP_UART_DMA_INVALID : app_uart.h
- APP_UART_EVT_ABORT_RX : app_uart.h
- APP_UART_EVT_ABORT_TX : app_uart.h
- APP_UART_EVT_ABORT_TXRX : app_uart.h
- APP_UART_EVT_ERROR : app_uart.h
- APP_UART_EVT_RX_DATA : app_uart.h
- APP_UART_EVT_TX_CPLT : app_uart.h
- APP_UART_ID_0 : app_uart.h
- APP_UART_ID_1 : app_uart.h
- APP_UART_ID_MAX : app_uart.h
- APP_UART_INVALID : app_uart.h