Classes | Macros | Typedefs | Functions
gr55xx_ll_xqspi.h File Reference

Header file containing functions prototypes of XQSPI LL library. More...

`#include "gr55xx.h"`
Include dependency graph for gr55xx_ll_xqspi.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Classes
struct | _ll_xqspi_init_t
| XQSPI init structures definition. More...

## Macros
#define | LL_XQSPI_MODE_XIP 0
| XIP mode More...
#define | LL_XQSPI_MODE_QSPI 1
| QSPI mode More...
#define | LL_XQSPI_XIP_CMD_READ 0x03
| Read mode More...
#define | LL_XQSPI_XIP_CMD_FAST_READ 0x0B
| Fast Read mode More...
#define | LL_XQSPI_XIP_CMD_DUAL_OUT_READ 0x3B
| Dual-Out Fast Read mode More...
#define | LL_XQSPI_XIP_CMD_DUAL_IO_READ 0xBB
| Dual-IO Fast Read mode More...
#define | LL_XQSPI_XIP_CMD_QUAD_OUT_READ 0x6B
| Quad-Out Fast Read mode More...
#define | LL_XQSPI_XIP_CMD_QUAD_IO_READ 0xEB
| Quad-IO Fast Read mode More...
#define | LL_XQSPI_XIP_SS0 (1UL << XQSPI_XIP_CFG_SS_Pos)
| Slave select 0. More...
#define | LL_XQSPI_XIP_SS1 (2UL << XQSPI_XIP_CFG_SS_Pos)
| Slave select 1. More...
#define | LL_XQSPI_XIP_SS2 (4UL << XQSPI_XIP_CFG_SS_Pos)
| Slave select 2. More...
#define | LL_XQSPI_XIP_SS3 (8UL << XQSPI_XIP_CFG_SS_Pos)
| Slave select 3. More...
#define | LL_XQSPI_XIP_ADDR_3BYTES 0x00000000UL
| Address command is 3 bytes More...
#define | LL_XQSPI_XIP_ADDR_4BYTES XQSPI_XIP_CFG_ADDR4
| Address command is 4 bytes More...
#define | LL_XQSPI_XIP_ENDIAN_BIG 0x00000000UL
| Read data in big endian More...
#define | LL_XQSPI_XIP_ENDIAN_LITTLE XQSPI_XIP_CFG_LE32
| Read data in little endian. More...
#define | LL_XQSPI_CACHE_DIS 0
| Cache OFF. More...
#define | LL_XQSPI_CACHE_EN 1
| Cache ON More...
#define | LL_XQSPI_CACHE_FIFO_NORMAL 0x00000000UL
| FIFO in normal mode. More...
#define | LL_XQSPI_CACHE_FIFO_CLEAR XQSPI_CACHE_CTRL0_FIFO
| FIFO in clear mode More...
#define | LL_XQSPI_CACHE_HITMISS_NORMAL 0x00000000UL
| Hit/Miss counters in normal mode. More...
#define | LL_XQSPI_CACHE_HITMISS_CLEAR XQSPI_CACHE_CTRL0_HITMISS
| Hit/Miss counters in clear mode More...
#define | LL_XQSPI_QSPI_STAT_RFTF XQSPI_QSPI_STAT_RXWMARK
| Rx FIFO watermark flag More...
#define | LL_XQSPI_QSPI_STAT_RFF XQSPI_QSPI_STAT_RXFULL
| Rx FIFO full flag More...
#define | LL_XQSPI_QSPI_STAT_RFE XQSPI_QSPI_STAT_RXEMPTY
| Rx FIFO empty flag More...
#define | LL_XQSPI_QSPI_STAT_TFTF XQSPI_QSPI_STAT_TXWMARK
| Tx FIFO watermark flag More...
#define | LL_XQSPI_QSPI_STAT_TFF XQSPI_QSPI_STAT_TXFULL
| Tx FIFO full flag More...
#define | LL_XQSPI_QSPI_STAT_TFE XQSPI_QSPI_STAT_TXEMPTY
| Tx FIFO empty flag More...
#define | LL_XQSPI_QSPI_STAT_BUSY XQSPI_QSPI_STAT_XFERIP
| Busy flag More...
#define | LL_XQSPI_QSPI_IM_DONE XQSPI_QSPI_XFER_DPULSE_Msk
| Transmite Done Interrupt enable More...
#define | LL_XQSPI_QSPI_IM_RFF XQSPI_QSPI_RX_FPULSE_Msk
| Receive FIFO Full Interrupt enable More...
#define | LL_XQSPI_QSPI_IM_RFTF XQSPI_QSPI_RX_WPULSE_Msk
| Receive FIFO Watermark Interrupt enable More...
#define | LL_XQSPI_QSPI_IM_TFTF XQSPI_QSPI_TX_WPULSE_Msk
| Transmit FIFO Watermark Interrupt enable More...
#define | LL_XQSPI_QSPI_IM_TFE XQSPI_QSPI_TX_EPULSE_Msk
| Transmit FIFO Empty Interrupt enable More...
#define | LL_XQSPI_QSPI_IS_DONE XQSPI_QSPI_XFER_DPULSE_Msk
| Transmite Done Interrupt flag More...
#define | LL_XQSPI_QSPI_IS_RFF XQSPI_QSPI_RX_FPULSE_Msk
| Receive FIFO Full Interrupt flag More...
#define | LL_XQSPI_QSPI_IS_RFTF XQSPI_QSPI_RX_WPULSE_Msk
| Receive FIFO Watermark Interrupt flag More...
#define | LL_XQSPI_QSPI_IS_TFTF XQSPI_QSPI_TX_WPULSE_Msk
| Transmit FIFO Watermark Interrupt flag More...
#define | LL_XQSPI_QSPI_IS_TFE XQSPI_QSPI_TX_EPULSE_Msk
| Transmit FIFO Empty Interrupt flag More...
#define | LL_XQSPI_QSPI_FIFO_WATERMARK_1_8 0UL
| FIFO depth/8 More...
#define | LL_XQSPI_QSPI_FIFO_WATERMARK_1_4 1UL
| FIFO depth/4 More...
#define | LL_XQSPI_QSPI_FIFO_WATERMARK_1_2 2UL
| FIFO depth/2 More...
#define | LL_XQSPI_QSPI_FIFO_WATERMARK_3_4 3UL
| FIFO depth*3/4 More...
#define | LL_XQSPI_QSPI_FIFO_DEPTH 16UL
| FIFO full depth More...
#define | LL_XQSPI_QSPI_FRF_SPI 0x00000000UL
| SPI frame format for transfer More...
#define | LL_XQSPI_QSPI_FRF_DUALSPI (2UL << XQSPI_QSPI_AUXCTRL_QMODE_Pos)
| Dual-SPI frame format for transfer. More...
#define | LL_XQSPI_QSPI_FRF_QUADSPI (3UL << XQSPI_QSPI_AUXCTRL_QMODE_Pos)
| Quad-SPI frame format for transfer. More...
#define | LL_XQSPI_QSPI_LSB 0x00000000UL
| LSB first for transfer. More...
#define | LL_XQSPI_QSPI_MSB XQSPI_QSPI_CTRL_MSB1ST
| MSB first for transfer. More...
#define | LL_XQSPI_QSPI_DATASIZE_4BIT 0x00000000UL
| Data length for XQSPI transfer: 4 bits. More...
#define | LL_XQSPI_QSPI_DATASIZE_8BIT (1UL << XQSPI_QSPI_AUXCTRL_BITSIZE_Pos)
| Data length for XQSPI transfer: 8 bits. More...
#define | LL_XQSPI_QSPI_DATASIZE_12BIT (2UL << XQSPI_QSPI_AUXCTRL_BITSIZE_Pos)
| Data length for XQSPI transfer: 12 bits. More...
#define | LL_XQSPI_QSPI_DATASIZE_16BIT (3UL << XQSPI_QSPI_AUXCTRL_BITSIZE_Pos)
| Data length for XQSPI transfer: 16 bits. More...
#define | LL_XQSPI_QSPI_DATASIZE_20BIT (4UL << XQSPI_QSPI_AUXCTRL_BITSIZE_Pos)
| Data length for XQSPI transfer: 20 bits. More...
#define | LL_XQSPI_QSPI_DATASIZE_24BIT (5UL << XQSPI_QSPI_AUXCTRL_BITSIZE_Pos)
| Data length for XQSPI transfer: 24 bits. More...
#define | LL_XQSPI_QSPI_DATASIZE_28BIT (6UL << XQSPI_QSPI_AUXCTRL_BITSIZE_Pos)
| Data length for XQSPI transfer: 28 bits. More...
#define | LL_XQSPI_QSPI_DATASIZE_32BIT (7UL << XQSPI_QSPI_AUXCTRL_BITSIZE_Pos)
| Data length for XQSPI transfer: 32 bits. More...
#define | LL_XQSPI_SCPHA_1EDGE 0
| First clock transition is the first data capture edge More...
#define | LL_XQSPI_SCPHA_2EDGE 1
| Second clock transition is the first data capture edge. More...
#define | LL_XQSPI_SCPOL_LOW 0
| Clock to 0 when idle. More...
#define | LL_XQSPI_SCPOL_HIGH 1
| Clock to 1 when idle. More...
#define | LL_XQSPI_BAUD_RATE_64M 0x00000000UL
| Clock to 64MHz. More...
#define | LL_XQSPI_BAUD_RATE_48M (1UL << AON_PWR_REG01_XF_SCK_CLK_SEL_Pos)
| Clock to 48MHz. More...
#define | LL_XQSPI_BAUD_RATE_32M (2UL << AON_PWR_REG01_XF_SCK_CLK_SEL_Pos)
| Clock to 32MHz. More...
#define | LL_XQSPI_BAUD_RATE_24M (3UL << AON_PWR_REG01_XF_SCK_CLK_SEL_Pos)
| Clock to 24MHz. More...
#define | LL_XQSPI_BAUD_RATE_16M (4UL << AON_PWR_REG01_XF_SCK_CLK_SEL_Pos)
| Clock to 16MHz. More...
#define | LL_XQSPI_ENABLE_PRESENT 0
| Enable Present Bypass More...
#define | LL_XQSPI_DISABLE_PRESENT 1
| Disable Present Bypass. More...
#define | LL_XQSPI_FLASH_WRITE_128BIT 0
| 128bits flash write More...
#define | LL_XQSPI_FLASH_WRITE_32BIT 1
| 32bits flash write More...
#define | LL_XQSPI_DEFAULT_CONFIG
| LL XQSPI InitStrcut default configuartion. More...
#define | LL_XQSPI_WriteReg(__instance__, __REG__, __VALUE__) WRITE_REG(__instance__->__REG__, (__VALUE__))
| Write a value in XQSPI register. More...
#define | LL_XQSPI_ReadReg(__instance__, __REG__) READ_REG(__instance__->__REG__)
| Read a value in XQSPI register. More...

## Typedefs
typedef struct _ll_xqspi_init_t | ll_xqspi_init_t
| XQSPI init structures definition. More...

## Functions
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_enable_cache (xqspi_regs_t *XQSPIx)
| Enable cache function. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_disable_cache (xqspi_regs_t *XQSPIx)
| Disable cache function. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_is_enabled_cache (xqspi_regs_t *XQSPIx)
| Check if cache function is enabled. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_enable_cache_flush (xqspi_regs_t *XQSPIx)
| Enable tag memory flush. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_disable_cache_flush (xqspi_regs_t *XQSPIx)
| Disable tag memory flush. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_is_enabled_cache_flush (xqspi_regs_t *XQSPIx)
| Check if tag memory flush is enabled. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_set_cache_fifo (xqspi_regs_t *XQSPIx, uint32_t mode)
| Set FIFO mode. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_cache_fifo (xqspi_regs_t *XQSPIx)
| Get FIFO mode. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_set_cache_hitmiss (xqspi_regs_t *XQSPIx, uint32_t mode)
| Set HIT/MISS mode. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_cache_hitmiss (xqspi_regs_t *XQSPIx)
| Get HIT/MISS mode. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_set_cache_dbgbus (xqspi_regs_t *XQSPIx, uint32_t sel)
| Set debugbus configurations signals. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_cache_dbgbus (xqspi_regs_t *XQSPIx)
| Get debugbus configurations signals. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_enable_cache_dbgmux (xqspi_regs_t *XQSPIx)
| Enable debug bus mux. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_disable_cache_dbgmux (xqspi_regs_t *XQSPIx)
| Disable debug bus mux. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_is_enabled_cache_dbgmux (xqspi_regs_t *XQSPIx)
| Check if debug bus mux is enabled. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_cache_hitcount (xqspi_regs_t *XQSPIx)
| Get hit counter. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_cache_misscount (xqspi_regs_t *XQSPIx)
| Get miss counter. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_cache_flag (xqspi_regs_t *XQSPIx)
| Get cache status. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_set_xip_cmd (xqspi_regs_t *XQSPIx, uint32_t cmd)
| Set read command. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_xip_cmd (xqspi_regs_t *XQSPIx)
| Get read command. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_enable_xip_hp (xqspi_regs_t *XQSPIx)
| Enable high performance mode. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_disable_xip_hp (xqspi_regs_t *XQSPIx)
| Disable high performance mode. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_is_enabled_xip_hp (xqspi_regs_t *XQSPIx)
| Check if high performance mode is enabled. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_set_xip_ss (xqspi_regs_t *XQSPIx, uint32_t ss)
| Set slave select. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_xip_ss (xqspi_regs_t *XQSPIx)
| Get slave select. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_set_xip_cpha (xqspi_regs_t *XQSPIx, uint32_t cpha)
| Set clock phase. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_xip_cpha (xqspi_regs_t *XQSPIx)
| Get clock phase. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_set_xip_cpol (xqspi_regs_t *XQSPIx, uint32_t cpol)
| Set clock polarity. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_xip_cpol (xqspi_regs_t *XQSPIx)
| Get clock polarity. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_set_xip_addr_size (xqspi_regs_t *XQSPIx, uint32_t size)
| Set address bytes in command. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_xip_addr_size (xqspi_regs_t *XQSPIx)
| Get address bytes in command. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_set_xip_endian (xqspi_regs_t *XQSPIx, uint32_t endian)
| Set endian in reading data. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_xip_endian (xqspi_regs_t *XQSPIx)
| Get endian in reading data. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_set_xip_hp_cmd (xqspi_regs_t *XQSPIx, uint32_t cmd)
| Set high performance command. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_xip_hp_cmd (xqspi_regs_t *XQSPIx)
| Get high performance command. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_set_xip_dummycycles (xqspi_regs_t *XQSPIx, uint32_t cycles)
| Set dummy cycles in command. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_xip_dummycycles (xqspi_regs_t *XQSPIx)
| Get dummy cycles in command. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_set_xip_dummy_hp (xqspi_regs_t *XQSPIx, uint32_t cycles)
| Set dummy cycles in high performance end. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_xip_dummy_hp (xqspi_regs_t *XQSPIx)
| Get dummy cycles in high performance end. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_enable_xip (xqspi_regs_t *XQSPIx)
| Enable XIP mode. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_disable_xip (xqspi_regs_t *XQSPIx)
| Disable XIP mode. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_is_enabled_xip (xqspi_regs_t *XQSPIx)
| Check if XIP mode is enabled. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_xip_flag (xqspi_regs_t *XQSPIx)
| Get XIP status. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_is_enabled_xip_it (xqspi_regs_t *XQSPIx)
| Check if XIP interrupt is enabled. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_flag_xip_it (xqspi_regs_t *XQSPIx)
| Get XIP interrupt flag. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_req_xip_it (xqspi_regs_t *XQSPIx)
| Get XIP interrupt request. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_enable_xip_it (xqspi_regs_t *XQSPIx)
| Set XIP interrupt enable. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_disable_xip_it (xqspi_regs_t *XQSPIx)
| Set XIP interrupt disable. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_qspi_transmit_data8 (xqspi_regs_t *XQSPIx, uint8_t tx_data)
| Write 8-bit in the data register. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_qspi_transmit_data16 (xqspi_regs_t *XQSPIx, uint16_t tx_data)
| Write 16-bit in the data register. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_qspi_transmit_data32 (xqspi_regs_t *XQSPIx, uint32_t tx_data)
| Write 32-bit in the data register. More...
SECTION_RAM_CODE __STATIC_INLINE uint8_t | ll_xqspi_qspi_receive_data8 (xqspi_regs_t *XQSPIx)
| Read 8 bits in the data register. More...
SECTION_RAM_CODE __STATIC_INLINE uint16_t | ll_xqspi_qspi_receive_data16 (xqspi_regs_t *XQSPIx)
| Read 16 bits in the data register. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_qspi_receive_data32 (xqspi_regs_t *XQSPIx)
| Read 32 bits in the data register. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_set_qspi_tft (xqspi_regs_t *XQSPIx, uint32_t threshold)
| Set TX FIFO threshold level. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_qspi_tft (xqspi_regs_t *XQSPIx)
| Get TX FIFO threshold level. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_set_qspi_rft (xqspi_regs_t *XQSPIx, uint32_t threshold)
| Set RX FIFO threshold level. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_qspi_rft (xqspi_regs_t *XQSPIx)
| Get RX FIFO threshold level. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_enable_qspi_dummy (xqspi_regs_t *XQSPIx)
| Enable dummy cycles. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_disable_qspi_dummy (xqspi_regs_t *XQSPIx)
| Disable dummy cycles. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_is_enabled_qspi_dummy (xqspi_regs_t *XQSPIx)
| Check if dummy cycles is enabled. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_enable_qspi_dma (xqspi_regs_t *XQSPIx)
| Enable DMA mode. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_disable_qspi_dma (xqspi_regs_t *XQSPIx)
| Disable DMA mode. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_is_enabled_qspi_dma (xqspi_regs_t *XQSPIx)
| Check if DMA mode is enabled. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_set_qspi_cpol (xqspi_regs_t *XQSPIx, uint32_t cpol)
| Set clock polarity. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_qspi_cpol (xqspi_regs_t *XQSPIx)
| Get clock polarity. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_set_qspi_cpha (xqspi_regs_t *XQSPIx, uint32_t cpha)
| Set clock phase. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_qspi_cpha (xqspi_regs_t *XQSPIx)
| Get clock phase. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_set_qspi_data_order (xqspi_regs_t *XQSPIx, uint32_t order)
| Set serial data order. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_qspi_data_order (xqspi_regs_t *XQSPIx)
| Get serial data order. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_enable_qspi_contxfer (xqspi_regs_t *XQSPIx)
| Enable continuous transfer mode. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_disable_qspi_contxfer (xqspi_regs_t *XQSPIx)
| Disable continuous transfer mode. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_is_enabled_qspi_contxfer (xqspi_regs_t *XQSPIx)
| Check if continuous transfer mode is enabled. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_enable_qspi_contxfer_extend (xqspi_regs_t *XQSPIx)
| Enable continuous transfer extend mode. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_disable_qspi_contxfer_extend (xqspi_regs_t *XQSPIx)
| Disable continuous transfer extend mode. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_is_enabled_qspi_contxfer_extend (xqspi_regs_t *XQSPIx)
| Check if continuous transfer extend mode is enabled. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_set_qspi_datasize (xqspi_regs_t *XQSPIx, uint32_t szie)
| Set data size. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_qspi_datasize (xqspi_regs_t *XQSPIx)
| Get data size. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_enable_inhibt_rx (xqspi_regs_t *XQSPIx)
| Enable inhibt data input to RX FIFO. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_disable_inhibt_rx (xqspi_regs_t *XQSPIx)
| Disable inhibt data input to RX FIFO. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_is_enabled_inhibt_rx (xqspi_regs_t *XQSPIx)
| Check if inhibt data input to RX FIFO is enabled. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_enable_inhibt_tx (xqspi_regs_t *XQSPIx)
| Enable inhibt data output to TX FIFO. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_disable_inhibt_tx (xqspi_regs_t *XQSPIx)
| Disable inhibt data output to TX FIFO. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_is_enabled_inhibt_tx (xqspi_regs_t *XQSPIx)
| Check if inhibt data input to TX FIFO is enabled. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_set_qspi_frf (xqspi_regs_t *XQSPIx, uint32_t format)
| Set frame format. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_qspi_frf (xqspi_regs_t *XQSPIx)
| Get frame format. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_qspi_status (xqspi_regs_t *XQSPIx)
| Get QSPI status. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_is_active_qspi_flag (xqspi_regs_t *XQSPIx, uint32_t flag)
| Check active flag. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_enable_qspi_ssout (xqspi_regs_t *XQSPIx, uint32_t ssout)
| Enable slave select output. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_disable_qspi_ssout (xqspi_regs_t *XQSPIx, uint32_t ssout)
| Disable slave select output. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_set_qspi_sspol (xqspi_regs_t *XQSPIx, uint32_t sspol)
| Set slave select output polarity. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_qspi_sspol (xqspi_regs_t *XQSPIx)
| Get slave select output polarity. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_qspi_tx_fifo_level (xqspi_regs_t *XQSPIx)
| Get FIFO Transmission Level. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_qspi_rx_fifo_level (xqspi_regs_t *XQSPIx)
| Get FIFO reception Level. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_enable_qspi_it (xqspi_regs_t *XQSPIx, uint32_t mask)
| Enable interrupt. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_disable_qspi_it (xqspi_regs_t *XQSPIx, uint32_t mask)
| Disable interrupt. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_is_enabled_qspi_it (xqspi_regs_t *XQSPIx, uint32_t mask)
| Check if interrupt is enabled. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_it_flag (xqspi_regs_t *XQSPIx)
| Get XQSPI interrupt flags. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_is_qspi_it_flag (xqspi_regs_t *XQSPIx, uint32_t flag)
| Check interrupt flag. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_clear_qspi_flag (xqspi_regs_t *XQSPIx, uint32_t flag)
| Clear interrupt flag. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_set_qspi_wait (xqspi_regs_t *XQSPIx, uint32_t wait)
| Set master inter-transfer delay. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_qspi_wait (xqspi_regs_t *XQSPIx)
| Get master inter-transfer delay. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_enable_qspi (xqspi_regs_t *XQSPIx)
| Enable QSPI. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_disable_qspi (xqspi_regs_t *XQSPIx)
| Disable QSPI. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_is_enabled_qspi (xqspi_regs_t *XQSPIx)
| Check if QSPI is enabled. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_set_flash_write (xqspi_regs_t *XQSPIx, uint32_t bits)
| Set QSPI Flash write bits. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_flash_write (xqspi_regs_t *XQSPIx)
| Get QSPI Flash write bits. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_set_present_bypass (xqspi_regs_t *XQSPIx, uint32_t bypass)
| Set QSPI Present Bypass. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_present_bypass (xqspi_regs_t *XQSPIx)
| Get QSPI Present Bypass. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_enable_exflash_power (void)
| Enable exflash power. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_disable_exflash_power (void)
| Disable exflash power. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_is_enable_exflash_power (void)
| Check if exflash power is enabled. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_set_qspi_speed (uint32_t speed)
| Set XQSPI serial clock. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_get_qspi_speed (void)
| Get XQSPI serial clock. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_enable_cache_retention (void)
| Enable cache data retention. More...
SECTION_RAM_CODE __STATIC_INLINE void | ll_xqspi_disable_cache_retention (void)
| Disable cache data retention. More...
SECTION_RAM_CODE __STATIC_INLINE uint32_t | ll_xqspi_is_enable_cache_retention (void)
| Check if tag memory retention is enabled. More...
error_status_t | ll_xqspi_deinit (xqspi_regs_t *XQSPIx)
| De-initialize XQSPI registers (Registers restored to their default values). More...
error_status_t | ll_xqspi_init (xqspi_regs_t *XQSPIx, ll_xqspi_init_t *p_xqspi_init)
| Initialize XQSPI registers according to the specified parameters in default. More...
void | ll_xqspi_struct_init (ll_xqspi_init_t *p_xqspi_init)
| Set each field of a ll_xqspi_init_t type structure to default value. More...

## Detailed Description

Header file containing functions prototypes of XQSPI LL library.

Author
  BLE SDK Team

Attention

  ##### Copyright (c) 2019 GOODIX

All rights reserved.

Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met: Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer. Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution. Neither the name of GOODIX nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission.

THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL COPYRIGHT HOLDERS AND CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.

Definition in file gr55xx_ll_xqspi.h.