Modules
XQSPI Exported Constants
Peripheral Driver » LL Driver » XQSPI » Defines
Collaboration diagram for XQSPI Exported Constants:

## Modules
| XQSPI work mode
| XIP read command
| Slave select
| Address bytes in command
| Read data endian mode
| XIP cache mode
| Cache FIFO mode
| Cache hit/miss counters mode
| QSPI Flags Defines
| Flags defines which can be used with LL_XQSPI_ReadReg function.
| QSPI interrupt Defines
| Interrupt defines which can be used with LL_XQSPI_ReadReg and LL_XQSPI_WriteReg functions.
| QSPI FIFO Watermark
| QSPI Frame Format
| QSPI Data Order
| QSPI Datawidth
| QSPI Clock Phase
| QSPI Clock Polarity
| QSPI Buad Rate
| QSPI Present Bypass
| QSPI Flash write bits
| InitStrcut default configuartion

## Detailed Description