Here is a list of all file members with links to the files they belong to:

### - d -

- delay_ms() : gr55xx_delay.h
- delay_us() : gr55xx_delay.h
- DELAY_US_DWT : gr55xx_delay.h
- DEVICE_BUSY : gr55xx_pwr.h
- DEVICE_IDLE : gr55xx_pwr.h
- dfu_ble_receive_data_process() : gr55xx_dfu.h
- dfu_ble_send_data_cmpl_process() : gr55xx_dfu.h
- dfu_ble_set_mtu_size() : gr55xx_dfu.h
- dfu_cmd_parse_state_reset() : gr55xx_dfu.h
- DFU_CONFIG_SPI_FLASH_DISABLE : gr55xx_dfu.h
- DFU_DUMP_FLASH_DISABLE : gr55xx_dfu.h
- DFU_ERASE_FLASH_DISABLE : gr55xx_dfu.h
- DFU_FRAME_RECEIVE_MAX_LENGTH : gr55xx_dfu.h
- DFU_IMG_INFO_PATTERN : gr55xx_dfu.h
- dfu_init() : gr55xx_dfu.h
- DFU_OPERATE_EFUSE_DISABLE : gr55xx_dfu.h
- DFU_OPERATE_NVDS_DISABLE : gr55xx_dfu.h
- DFU_OPERATE_REG_DISABLE : gr55xx_dfu.h
- DFU_OPERATE_SYSTEM_INFO_DISABLE : gr55xx_dfu.h
- DFU_READ_RAM_DISABLE : gr55xx_dfu.h
- dfu_receive_cmd_handler_t : gr55xx_dfu.h
- dfu_schedule() : gr55xx_dfu.h
- dfu_set_cmd_handler() : gr55xx_dfu.h
- dfu_set_disable_cmd() : gr55xx_dfu.h
- dfu_spi_flash_func_config() : gr55xx_dfu.h
- dfu_uart_receive_data_process() : gr55xx_dfu.h
- DFU_UPDAE_FLASH_DISABLE : gr55xx_dfu.h
- DFU_WRITE_RAM_DISABLE : gr55xx_dfu.h
- DMA0_REQUEST_I2C0_RX : gr55xx_hal_dma.h
- DMA0_REQUEST_I2C0_TX : gr55xx_hal_dma.h
- DMA0_REQUEST_I2C1_RX : gr55xx_hal_dma.h
- DMA0_REQUEST_I2C1_TX : gr55xx_hal_dma.h
- DMA0_REQUEST_I2S_M_RX : gr55xx_hal_dma.h
- DMA0_REQUEST_I2S_M_TX : gr55xx_hal_dma.h
- DMA0_REQUEST_I2S_S_RX : gr55xx_hal_dma.h
- DMA0_REQUEST_I2S_S_TX : gr55xx_hal_dma.h
- DMA0_REQUEST_MEM : gr55xx_hal_dma.h
- DMA0_REQUEST_QSPI0_RX : gr55xx_hal_dma.h
- DMA0_REQUEST_QSPI0_TX : gr55xx_hal_dma.h
- DMA0_REQUEST_QSPI1_RX : gr55xx_hal_dma.h
- DMA0_REQUEST_QSPI1_TX : gr55xx_hal_dma.h
- DMA0_REQUEST_SNSADC : gr55xx_hal_dma.h
- DMA0_REQUEST_SPIM_RX : gr55xx_hal_dma.h
- DMA0_REQUEST_SPIM_TX : gr55xx_hal_dma.h
- DMA0_REQUEST_SPIS_RX : gr55xx_hal_dma.h
- DMA0_REQUEST_SPIS_TX : gr55xx_hal_dma.h
- DMA0_REQUEST_UART0_RX : gr55xx_hal_dma.h
- DMA0_REQUEST_UART0_TX : gr55xx_hal_dma.h
- DMA_Channel0 : gr55xx_hal_dma.h
- DMA_Channel1 : gr55xx_hal_dma.h
- DMA_Channel2 : gr55xx_hal_dma.h
- DMA_Channel3 : gr55xx_hal_dma.h
- DMA_Channel4 : gr55xx_hal_dma.h
- DMA_Channel5 : gr55xx_hal_dma.h
- DMA_Channel6 : gr55xx_hal_dma.h
- DMA_Channel7 : gr55xx_hal_dma.h
- dma_channel_t : gr55xx_hal_dma.h
- DMA_CIRCULAR : gr55xx_hal_dma.h
- DMA_DDATAALIGN_BYTE : gr55xx_hal_dma.h
- DMA_DDATAALIGN_HALFWORD : gr55xx_hal_dma.h
- DMA_DDATAALIGN_WORD : gr55xx_hal_dma.h
- DMA_DST_DECREMENT : gr55xx_hal_dma.h
- DMA_DST_INCREMENT : gr55xx_hal_dma.h
- DMA_DST_NO_CHANGE : gr55xx_hal_dma.h
- dma_handle_t : gr55xx_hal_dma.h
- dma_id_t : app_dma.h
- dma_init_t : gr55xx_hal_dma.h
- DMA_LLP_BLOCKS_FOR_BLIT : app_qspi_user_config.h
- DMA_LLP_BLOCKS_FOR_WRITE : app_qspi_user_config.h
- DMA_MEMORY_TO_MEMORY : gr55xx_hal_dma.h
- DMA_MEMORY_TO_PERIPH : gr55xx_hal_dma.h
- DMA_NORMAL : gr55xx_hal_dma.h
- DMA_PERIPH_TO_MEMORY : gr55xx_hal_dma.h
- DMA_PERIPH_TO_PERIPH : gr55xx_hal_dma.h
- DMA_PRIORITY_HIGH : gr55xx_hal_dma.h
- DMA_PRIORITY_LOW : gr55xx_hal_dma.h
- DMA_PRIORITY_MEDIUM : gr55xx_hal_dma.h
- DMA_PRIORITY_VERY_HIGH : gr55xx_hal_dma.h
- DMA_REQUEST_I2C0_RX : gr55xx_hal_dma.h
- DMA_REQUEST_I2C0_TX : gr55xx_hal_dma.h
- DMA_REQUEST_I2C1_RX : gr55xx_hal_dma.h
- DMA_REQUEST_I2C1_TX : gr55xx_hal_dma.h
- DMA_REQUEST_I2S_M_RX : gr55xx_hal_dma.h
- DMA_REQUEST_I2S_M_TX : gr55xx_hal_dma.h
- DMA_REQUEST_I2S_S_RX : gr55xx_hal_dma.h
- DMA_REQUEST_I2S_S_TX : gr55xx_hal_dma.h
- DMA_REQUEST_MEM : gr55xx_hal_dma.h
- DMA_REQUEST_QSPI0_RX : gr55xx_hal_dma.h
- DMA_REQUEST_QSPI0_TX : gr55xx_hal_dma.h
- DMA_REQUEST_QSPI1_RX : gr55xx_hal_dma.h
- DMA_REQUEST_QSPI1_TX : gr55xx_hal_dma.h
- DMA_REQUEST_SNSADC : gr55xx_hal_dma.h
- DMA_REQUEST_SPIM_RX : gr55xx_hal_dma.h
- DMA_REQUEST_SPIM_TX : gr55xx_hal_dma.h
- DMA_REQUEST_SPIS_RX : gr55xx_hal_dma.h
- DMA_REQUEST_SPIS_TX : gr55xx_hal_dma.h
- DMA_REQUEST_UART0_RX : gr55xx_hal_dma.h
- DMA_REQUEST_UART0_TX : gr55xx_hal_dma.h
- DMA_SDATAALIGN_BYTE : gr55xx_hal_dma.h
- DMA_SDATAALIGN_HALFWORD : gr55xx_hal_dma.h
- DMA_SDATAALIGN_WORD : gr55xx_hal_dma.h
- DMA_SRC_DECREMENT : gr55xx_hal_dma.h
- DMA_SRC_INCREMENT : gr55xx_hal_dma.h
- DMA_SRC_NO_CHANGE : gr55xx_hal_dma.h
- DUAL_TIMER_COUNTERMODE_LOOP : gr55xx_hal_dual_tim.h
- DUAL_TIMER_COUNTERMODE_ONESHOT : gr55xx_hal_dual_tim.h
- DUAL_TIMER_DEFAULT_CONFIG : gr55xx_ll_dual_tim.h
- dual_timer_handle_t : gr55xx_hal_dual_tim.h
- dual_timer_init_t : gr55xx_hal_dual_tim.h
- DUAL_TIMER_PRESCALER_DIV0 : gr55xx_hal_dual_tim.h
- DUAL_TIMER_PRESCALER_DIV16 : gr55xx_hal_dual_tim.h
- DUAL_TIMER_PRESCALER_DIV256 : gr55xx_hal_dual_tim.h