Public Attributes | List of all members
ble_gap_adv_second_cfg_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Management » Structures

Configuration for advertising on secondary channel. More...

`#include <ble_gapm.h>`

## Public Attributes
uint8_t | max_skip
| Maximum number of advertising events the controller can skip before sending the AUX_ADV_IND packets. More...
ble_gap_le_phy_value_t | phy
| Indicate on which PHY secondary advertising has to be performed. More...
uint8_t | adv_sid
| Advertising SID. More...

## Detailed Description

Configuration for advertising on secondary channel.

Definition at line 573 of file ble_gapm.h.

## Member Data Documentation

## ◆ adv_sid

uint8_t ble_gap_adv_second_cfg_t::adv_sid

Advertising SID.

Allowed range is 0x00 to 0x0F.

Definition at line 577 of file ble_gapm.h.

## ◆ max_skip

uint8_t ble_gap_adv_second_cfg_t::max_skip

Maximum number of advertising events the controller can skip before sending the AUX_ADV_IND packets.

The range is 0x00 to 0xFF. 0x00 means that AUX_ADV_IND PDUs shall be sent prior to each advertising events.

Definition at line 575 of file ble_gapm.h.

## ◆ phy

ble_gap_le_phy_value_t ble_gap_adv_second_cfg_t::phy

Indicate on which PHY secondary advertising has to be performed.

See enum ble_gap_le_phy_value_t.

Definition at line 576 of file ble_gapm.h.

The documentation for this struct was generated from the following file:

- ble_gapm.h