### - a -

- aon_gpio_pin_state_t : gr55xx_hal_aon_gpio.h
- app_adc_dma_state_t : app_adc.h
- app_adc_evt_type_t : app_adc.h
- app_adc_state_t : app_adc.h
- app_aes_evt_type_t : app_aes.h
- app_aes_mode_t : app_aes.h
- app_aes_state_t : app_aes.h
- app_aon_wdt_state_t : app_aon_wdt.h
- app_comp_evt_t : app_comp.h
- app_comp_state_t : app_comp.h
- app_dma_evt_type_t : app_dma.h
- app_dma_state_t : app_dma.h
- app_dual_tim_evt_t : app_dual_tim.h
- app_dual_tim_id_t : app_dual_tim.h
- app_dual_tim_state_t : app_dual_tim.h
- app_hmac_evt_type_t : app_hmac.h
- app_hmac_state_t : app_hmac.h
- app_hmac_type_t : app_hmac.h
- app_i2c_dma_state_t : app_i2c.h
- app_i2c_evt_type_t : app_i2c.h
- app_i2c_id_t : app_i2c.h
- app_i2c_role_t : app_i2c.h
- app_i2c_state_t : app_i2c.h
- app_i2s_dma_state_t : app_i2s.h
- app_i2s_evt_type_t : app_i2s.h
- app_i2s_id_t : app_i2s.h
- app_i2s_state_t : app_i2s.h
- app_io_input_type_t : app_io.h
- app_io_mode_t : app_io.h
- app_io_mux_t : app_io.h
- app_io_pin_state_t : app_io.h
- app_io_pull_t : app_io.h
- app_io_speed_t : app_io.h
- app_io_strength_t : app_io.h
- app_io_type_t : app_io.h
- app_iso7816_evt_type_t : app_iso7816.h
- app_iso7816_mode_t : app_iso7816.h
- app_iso7816_state_t : app_iso7816.h
- app_pkc_evt_type_t : app_pkc.h
- app_pkc_state_t : app_pkc.h
- app_pkc_type_t : app_pkc.h
- app_pwm_active_channel_t : app_pwm.h
- app_pwm_id_t : app_pwm.h
- app_pwm_module_state_t : app_pwm.h
- app_pwm_state_t : app_pwm.h
- app_qspi_dma_state_t : app_qspi.h
- app_qspi_evt_type_t : app_qspi.h
- app_qspi_id_t : app_qspi.h
- app_qspi_state_t : app_qspi.h
- app_rng_evt_type_t : app_rng.h
- app_rng_state_t : app_rng.h
- app_rng_type_t : app_rng.h
- app_rtc_evt_type_t : app_rtc.h
- app_spi_dma_state_t : app_spi.h
- app_spi_evt_type_t : app_spi.h
- app_spi_id_t : app_spi.h
- app_spi_state_t : app_spi.h
- app_tim_evt_t : app_tim.h
- app_tim_id_t : app_tim.h
- app_tim_state_t : app_tim.h
- app_uart_dma_state_t : app_uart.h
- app_uart_evt_type_t : app_uart.h
- app_uart_id_t : app_uart.h
- app_uart_state_t : app_uart.h

### - b -

- ble_att_format_t : ble_att.h
- ble_att_uuid_t : ble_att.h
- BLE_COMMON_EVTS : ble_event.h
- ble_gap_actv_role_t : ble_gapm.h
- ble_gap_actv_type_t : ble_gapm.h
- ble_gap_ad_type_t : ble_gapm.h
- ble_gap_adv_data_type_t : ble_gapm.h
- ble_gap_adv_filter_policy_t : ble_gapm.h
- ble_gap_adv_flags_t : ble_gapm.h
- ble_gap_adv_mode_t : ble_gapm.h
- ble_gap_adv_prop_pos_t : ble_gapm.h
- ble_gap_adv_prop_t : ble_gapm.h
- ble_gap_adv_report_info_t : ble_gapm.h
- ble_gap_adv_report_type_t : ble_gapm.h
- ble_gap_adv_type_t : ble_gapm.h
- ble_gap_clk_acc_t : ble_gapm.h
- ble_gap_dev_info_get_type_t : ble_gapm.h
- ble_gap_dev_name_write_perm_t : ble_gapm.h
- ble_gap_disc_mode_t : ble_gapm.h
- ble_gap_disconn_reason_t : ble_gapc.h
- ble_gap_ext_scan_dup_filt_policy_t : ble_gapm.h
- ble_gap_ext_scan_type_t : ble_gapm.h
- ble_gap_get_conn_info_op_t : ble_gapc.h
- ble_gap_get_peer_info_op_t : ble_gapc.h
- ble_gap_init_prop_t : ble_gapm.h
- ble_gap_init_type_t : ble_gapm.h
- ble_gap_le_phy_value_t : ble_gapm.h
- ble_gap_ll_role_type_t : ble_gapc.h
- ble_gap_own_addr_t : ble_gapm.h
- ble_gap_param_set_op_id_t : ble_gapc.h
- ble_gap_per_sync_type_t : ble_gapm.h
- ble_gap_privacy_mode_t : ble_gapm.h
- ble_gap_psm_manager_op_id_t : ble_gapc.h
- ble_gap_role_t : ble_gapm.h
- ble_gap_rslv_addr_read_op_id_t : ble_gapm.h
- ble_gap_scan_dup_filt_policy_t : ble_gapm.h
- ble_gap_scan_mode_t : ble_gapm.h
- ble_gap_scan_prop_t : ble_gapm.h
- ble_gap_scan_type_t : ble_gapm.h
- ble_gap_sec_lvl_type_t : ble_gapm.h
- ble_gap_stopped_reason_t : ble_gapm.h
- BLE_GAPC_EVTS : ble_event.h
- BLE_GAPM_EVTS : ble_event.h
- BLE_GATT_COMMON_EVTS : ble_event.h
- ble_gatt_evt_type_t : ble_gatt.h
- ble_gattc_attr_type_t : ble_gattc.h
- BLE_GATTC_EVTS : ble_event.h
- BLE_GATTS_EVTS : ble_event.h
- ble_gatts_service_type_t : ble_gatts.h
- BLE_L2CAP_EVTS : ble_event.h
- ble_l2cap_lecb_disconn_reason_t : ble_l2cap.h
- ble_rf_match_circuit_t : ble.h
- ble_rf_tx_mode_t : ble.h
- ble_sec_enc_req_type_t : ble_sec.h
- BLE_SEC_EVTS : ble_event.h
- ble_sec_io_cap_t : ble_sec.h
- ble_sec_key_missing_reason_t : ble_sec.h
- ble_sec_keypress_notify_t : ble_sec.h
- ble_sec_mode_level_t : ble_sec.h
- ble_sec_tk_type_t : ble_sec.h
- boot_mode_t : gr55xx_pwr.h

### - c -

- cgc_clk_state_t : gr55xx_hal_cgc.h

### - d -

- dma_channel_t : gr55xx_hal_dma.h

### - f -

- fpb_mode_t : gr55xx_fpb.h
- fpb_state_t : gr55xx_fpb.h

### - g -

- gpio_pin_state_t : gr55xx_hal_gpio.h

### - h -

- hal_adc_state_t : gr55xx_hal_adc.h
- hal_aes_state_t : gr55xx_hal_aes.h
- hal_calender_state_t : gr55xx_hal_calendar.h
- hal_comp_state_t : gr55xx_hal_comp.h
- hal_dma_callback_id_t : gr55xx_hal_dma.h
- hal_dma_state_t : gr55xx_hal_dma.h
- hal_dual_timer_state_t : gr55xx_hal_dual_tim.h
- hal_eflash_security : gr55xx_hal_exflash.h
- hal_efuse_state_t : gr55xx_hal_efuse.h
- hal_exflash_state_t : gr55xx_hal_exflash.h
- hal_hmac_state_t : gr55xx_hal_hmac.h
- hal_i2c_mode_t : gr55xx_hal_i2c.h
- hal_i2c_state_t : gr55xx_hal_i2c.h
- hal_i2s_state_t : gr55xx_hal_i2s.h
- hal_iso7816_state_t : gr55xx_hal_iso7816.h
- hal_lock_t : gr55xx_hal_def.h
- hal_pkc_state_t : gr55xx_hal_pkc.h
- hal_pwm_active_channel_t : gr55xx_hal_pwm.h
- hal_pwm_state_t : gr55xx_hal_pwm.h
- hal_qspi_state_t : gr55xx_hal_qspi.h
- hal_rng_state_t : gr55xx_hal_rng.h
- hal_spi_state_t : gr55xx_hal_spi.h
- hal_status_t : gr55xx_hal_def.h
- hal_timer_state_t : gr55xx_hal_tim.h
- hal_uart_state_t : gr55xx_hal_uart.h
- hal_xqspi_state_t : gr55xx_hal_xqspi.h

### - m -

- mem_power_t : platform_sdk.h
- msio_pad_t : gr55xx_ll_msio.h
- msio_pin_state_t : gr55xx_hal_msio.h

### - n -

- notify_timer_event_t : gr55xx_pwr.h
- NVDS_STATUS : gr55xx_nvds.h

### - p -

- package_type_t : gr55xx_sys.h
- PROTOCOL_MODE : ble_lcp.h
- pwr_mgmt_dev_state_t : gr55xx_pwr.h
- pwr_mgmt_mode_t : gr55xx_pwr.h

### - r -

- run_mode_t : platform_sdk.h

### - s -

- sdk_clock_type_t : platform_sdk.h
- sram_size_t : gr55xx_sys.h

### - w -

- wakeup_priority_t : app_drv_config.h