Public Attributes | List of all members
ble_gap_scan_wd_op_param_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Management » Structures

Scan Window operation parameters. More...

`#include <ble_gapm.h>`

## Public Attributes
uint16_t | scan_intv
| Scan interval between 0x0004 and 0xFFFF in 0.625 ms (range: 2.5 ms to 40.959375s). More...
uint16_t | scan_wd
| Scan window between 0x0004 and 0xFFFF in 0.625 ms (range: 2.5 ms to 40.959375s). More...

## Detailed Description

Scan Window operation parameters.

Definition at line 639 of file ble_gapm.h.

## Member Data Documentation

## ◆ scan_intv

uint16_t ble_gap_scan_wd_op_param_t::scan_intv

Scan interval between 0x0004 and 0xFFFF in 0.625 ms (range: 2.5 ms to 40.959375s).

Definition at line 641 of file ble_gapm.h.

## ◆ scan_wd

uint16_t ble_gap_scan_wd_op_param_t::scan_wd

Scan window between 0x0004 and 0xFFFF in 0.625 ms (range: 2.5 ms to 40.959375s).

Definition at line 642 of file ble_gapm.h.

The documentation for this struct was generated from the following file:

- ble_gapm.h