Public Attributes | List of all members
ble_gap_adv_period_cfg_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Management » Structures

Configuration for periodic advertising. More...

`#include <ble_gapm.h>`

## Public Attributes
uint16_t | adv_intv_min
| Minimum advertising interval (in unit of 1.25 ms). More...
uint16_t | adv_intv_max
| Maximum advertising interval (in unit of 1.25 ms). More...

## Detailed Description

Configuration for periodic advertising.

Definition at line 583 of file ble_gapm.h.

## Member Data Documentation

## ◆ adv_intv_max

uint16_t ble_gap_adv_period_cfg_t::adv_intv_max

Maximum advertising interval (in unit of 1.25 ms).

Must be greater than 20 ms.

Definition at line 586 of file ble_gapm.h.

## ◆ adv_intv_min

uint16_t ble_gap_adv_period_cfg_t::adv_intv_min

Minimum advertising interval (in unit of 1.25 ms).

Must be greater than 20 ms.

Definition at line 585 of file ble_gapm.h.

The documentation for this struct was generated from the following file:

- ble_gapm.h