Modules | Macros
Defines
SYSTEM » Device Firmware Update
Collaboration diagram for Defines:

## Modules
| DFU cmd disable option (bitmask)

## Macros
#define | DFU_FRAME_RECEIVE_MAX_LENGTH 2048
| The max length of received data is 2048 bytes. More...
#define | DFU_IMG_INFO_PATTERN 0x4744
| The pattern of image info. More...

## Detailed Description

## Macro Definition Documentation

## ◆ DFU_FRAME_RECEIVE_MAX_LENGTH

#define DFU_FRAME_RECEIVE_MAX_LENGTH 2048

The max length of received data is 2048 bytes.

Definition at line 56 of file gr55xx_dfu.h.

## ◆ DFU_IMG_INFO_PATTERN

#define DFU_IMG_INFO_PATTERN 0x4744

The pattern of image info.

Definition at line 57 of file gr55xx_dfu.h.