Public Attributes | List of all members
ble_gap_evt_conn_param_update_req_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

Connection parameter update request event for BLE_GAPC_EVT_CONN_PARAM_UPDATE_REQ. More...

`#include <ble_gapc.h>`

## Public Attributes
uint16_t | interval_min
| Minimum value for the connection interval. More...
uint16_t | interval_max
| Maximum value for the connection interval. More...
uint16_t | slave_latency
| Slave latency for the connection in number of connection events. More...
uint16_t | sup_timeout
| Supervision timeout for the LE link. More...

## Detailed Description

Connection parameter update request event for BLE_GAPC_EVT_CONN_PARAM_UPDATE_REQ.

Definition at line 420 of file ble_gapc.h.

## Member Data Documentation

## ◆ interval_max

uint16_t ble_gap_evt_conn_param_update_req_t::interval_max

Maximum value for the connection interval.

This shall be greater than or equal to Conn_Interval_Min. Range: 0x0006 to 0x0C80, unit: 1.25 ms, time range: 7.5 ms to 4 s.

Definition at line 424 of file ble_gapc.h.

## ◆ interval_min

uint16_t ble_gap_evt_conn_param_update_req_t::interval_min

Minimum value for the connection interval.

This shall be less than or equal to Conn_Interval_Max. Range: 0x0006 to 0x0C80, unit: 1.25 ms, time range: 7.5 ms to 4 s

Definition at line 422 of file ble_gapc.h.

## ◆ slave_latency

uint16_t ble_gap_evt_conn_param_update_req_t::slave_latency

Slave latency for the connection in number of connection events.

Range: 0x0000 to 0x01F3.

Definition at line 426 of file ble_gapc.h.

## ◆ sup_timeout

uint16_t ble_gap_evt_conn_param_update_req_t::sup_timeout

Supervision timeout for the LE link.

Range: 0x000A to 0x0C80, unit: 10 ms, time range: 100 ms to 32 s.

Definition at line 427 of file ble_gapc.h.

The documentation for this struct was generated from the following file:

- ble_gapc.h