Macros
Defines
Peripheral Driver » APP DRIVER » DRIVER CONFIG
Collaboration diagram for Defines:

## Macros
#define | APP_DRIVER_ADC_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH
| APP driver peripheral priority define. More...
#define | APP_DRIVER_AES_WAPEUP_PRIORITY WAPEUP_PRIORITY_MID
| AES Wakeup priority Mid. More...
#define | APP_DRIVER_COMP_WAPEUP_PRIORITY WAPEUP_PRIORITY_LOW
| COMP Wakeup priority Low. More...
#define | APP_DRIVER_DUAL_TIM_WAPEUP_PRIORITY WAPEUP_PRIORITY_MID
| DUAL TIM Wakeup priority Mid. More...
#define | APP_DRIVER_DMA_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH
| DMA Wakeup priority High. More...
#define | APP_DRIVER_GPIOTE_WAPEUP_PRIORITY WAPEUP_PRIORITY_LOW
| GPIOTE Wakeup priority Low. More...
#define | APP_DRIVER_SYSTICK_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH
| SysTick Wakeup priority High. More...
#define | APP_DRIVER_UART_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH
| Uart Wakeup priority High. More...
#define | APP_DRIVER_HMAC_WAPEUP_PRIORITY WAPEUP_PRIORITY_MID
| Hmac Wakeup priority Mid. More...
#define | APP_DRIVER_I2C_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH
| I2C Wakeup priority High. More...
#define | APP_DRIVER_I2S_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH
| I2S Wakeup priority High. More...
#define | APP_DRIVER_QSPI_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH
| QSPI Wakeup priority High. More...
#define | APP_DRIVER_RNG_WAPEUP_PRIORITY WAPEUP_PRIORITY_MID
| RNG Wakeup priority Mid. More...
#define | APP_DRIVER_SPI_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH
| SPI Wakeup priority High. More...
#define | APP_DRIVER_TIM_WAPEUP_PRIORITY WAPEUP_PRIORITY_MID
| TIM Wakeup priority Mid. More...
#define | APP_DRIVER_PWM_WAPEUP_PRIORITY WAPEUP_PRIORITY_MID
| PWM Wakeup priority Mid. More...
#define | APP_DRIVER_ISO7816_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH
| ISO7816 Wakeup priority High. More...
#define | APP_DRIVER_PKC_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH
| PKC Wakeup priority High. More...

## Detailed Description

## Macro Definition Documentation

## ◆ APP_DRIVER_ADC_WAPEUP_PRIORITY

#define APP_DRIVER_ADC_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH

APP driver peripheral priority define.

ADC Wakeup priority High

Definition at line 90 of file app_drv_config.h.

## ◆ APP_DRIVER_AES_WAPEUP_PRIORITY

#define APP_DRIVER_AES_WAPEUP_PRIORITY WAPEUP_PRIORITY_MID

AES Wakeup priority Mid.

Definition at line 94 of file app_drv_config.h.

## ◆ APP_DRIVER_COMP_WAPEUP_PRIORITY

#define APP_DRIVER_COMP_WAPEUP_PRIORITY WAPEUP_PRIORITY_LOW

COMP Wakeup priority Low.

Definition at line 98 of file app_drv_config.h.

## ◆ APP_DRIVER_DMA_WAPEUP_PRIORITY

#define APP_DRIVER_DMA_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH

DMA Wakeup priority High.

Definition at line 106 of file app_drv_config.h.

## ◆ APP_DRIVER_DUAL_TIM_WAPEUP_PRIORITY

#define APP_DRIVER_DUAL_TIM_WAPEUP_PRIORITY WAPEUP_PRIORITY_MID

DUAL TIM Wakeup priority Mid.

Definition at line 102 of file app_drv_config.h.

## ◆ APP_DRIVER_GPIOTE_WAPEUP_PRIORITY

#define APP_DRIVER_GPIOTE_WAPEUP_PRIORITY WAPEUP_PRIORITY_LOW

GPIOTE Wakeup priority Low.

Definition at line 110 of file app_drv_config.h.

## ◆ APP_DRIVER_HMAC_WAPEUP_PRIORITY

#define APP_DRIVER_HMAC_WAPEUP_PRIORITY WAPEUP_PRIORITY_MID

Hmac Wakeup priority Mid.

Definition at line 122 of file app_drv_config.h.

## ◆ APP_DRIVER_I2C_WAPEUP_PRIORITY

#define APP_DRIVER_I2C_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH

I2C Wakeup priority High.

Definition at line 126 of file app_drv_config.h.

## ◆ APP_DRIVER_I2S_WAPEUP_PRIORITY

#define APP_DRIVER_I2S_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH

I2S Wakeup priority High.

Definition at line 130 of file app_drv_config.h.

## ◆ APP_DRIVER_ISO7816_WAPEUP_PRIORITY

#define APP_DRIVER_ISO7816_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH

ISO7816 Wakeup priority High.

Definition at line 154 of file app_drv_config.h.

## ◆ APP_DRIVER_PKC_WAPEUP_PRIORITY

#define APP_DRIVER_PKC_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH

PKC Wakeup priority High.

Definition at line 158 of file app_drv_config.h.

## ◆ APP_DRIVER_PWM_WAPEUP_PRIORITY

#define APP_DRIVER_PWM_WAPEUP_PRIORITY WAPEUP_PRIORITY_MID

PWM Wakeup priority Mid.

Definition at line 150 of file app_drv_config.h.

## ◆ APP_DRIVER_QSPI_WAPEUP_PRIORITY

#define APP_DRIVER_QSPI_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH

QSPI Wakeup priority High.

Definition at line 134 of file app_drv_config.h.

## ◆ APP_DRIVER_RNG_WAPEUP_PRIORITY

#define APP_DRIVER_RNG_WAPEUP_PRIORITY WAPEUP_PRIORITY_MID

RNG Wakeup priority Mid.

Definition at line 138 of file app_drv_config.h.

## ◆ APP_DRIVER_SPI_WAPEUP_PRIORITY

#define APP_DRIVER_SPI_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH

SPI Wakeup priority High.

Definition at line 142 of file app_drv_config.h.

## ◆ APP_DRIVER_SYSTICK_WAPEUP_PRIORITY

#define APP_DRIVER_SYSTICK_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH

SysTick Wakeup priority High.

Definition at line 114 of file app_drv_config.h.

## ◆ APP_DRIVER_TIM_WAPEUP_PRIORITY

#define APP_DRIVER_TIM_WAPEUP_PRIORITY WAPEUP_PRIORITY_MID

TIM Wakeup priority Mid.

Definition at line 146 of file app_drv_config.h.

## ◆ APP_DRIVER_UART_WAPEUP_PRIORITY

#define APP_DRIVER_UART_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH

Uart Wakeup priority High.

Definition at line 118 of file app_drv_config.h.