### - w -

- wait_cycles : _ll_qspi_init_t
- wait_time : _ll_iso7816_init , iso7816_init_t
- wdt_msp_deinit : _hal_wdt_callback
- wdt_msp_init : _hal_wdt_callback
- wdt_period_elapsed_callback : _hal_wdt_callback
- week : _calendar_time
- wfi_clk : _cgc_init
- wfi_clk0 : _ll_cgc_init_t
- wfi_clk1 : _ll_cgc_init_t
- wfi_clk2 : _ll_cgc_init_t
- window : ble_gap_scan_param_t
- work_mode : _xqspi_init_t
- write : hci_uart_call_t
- write_fifo : _i2s_handle , _qspi_handle , _spi_handle
- write_req : ble_gatts_evt_t
- write_rsp : ble_gattc_evt_t
- ws : app_i2s_pin_cfg_t