Functions
IRQ Handler and Callbacks
Peripheral Driver » HAL Driver » PWR » Functions

IRQ Handler and Callbacks functions. More...

Collaboration diagram for IRQ Handler and Callbacks:

## Functions
void | hal_pwr_sleep_timer_irq_handler (void)
| Handle PWR Sleep Timer interrupt request. More...
void | hal_pwr_sleep_timer_elapsed_callback (void)
| PWR Sleep Timer Elapsed callback. More...

## Detailed Description

IRQ Handler and Callbacks functions.

## Function Documentation

## ◆ hal_pwr_sleep_timer_elapsed_callback()

void hal_pwr_sleep_timer_elapsed_callback | ( | void |  | ) |

PWR Sleep Timer Elapsed callback.

Note
  Only available on GR5515_C and later versions. This function should not be modified. When the callback is needed, the hal_pwr_sleep_timer_elapsed_callback can be implemented in the user file.

## ◆ hal_pwr_sleep_timer_irq_handler()

void hal_pwr_sleep_timer_irq_handler | ( | void |  | ) |

Handle PWR Sleep Timer interrupt request.

Note
  Only available on GR5515_C and later versions.